- Top
- Shooting
- Viewfinder status display
- Zebra patterns display

# Zebra patterns display

The camera can display two types of zebra patterns.

When the <ZEBRA> switch of the viewfinder is set to <ON>, the zebra pattern currently set in the menu is displayed on the viewfinder screen.

Zebra patterns can also be displayed in the video of the monitor output terminal (<SDI OUT2>, <VIDEO OUT>, <HDMI OUT>) according to settings.

The level for displaying zebra patterns can be set in the main menu → [VF] → [VF DISPLAY].

Item | Description of settings
--- | ---
[ZEBRA1 DETECT] | Sets the level of zebra pattern 1 tilting to the right. [0%]…[109%] Factory setting: [70%]
[ZEBRA2 DETECT] | Sets the level of zebra pattern 2 tilting to the left. [0%]…[109%] Factory setting: [85%]
[ZEBRA2] | Selects the type of [ZEBRA2]. [ON], [SPOT], [OFF] Factory setting: [SPOT]

[SPOT]: The image level from the setting value of [ZEBRA1 DETECT] to the setting value of [ZEBRA2 DETECT] is displayed in the zebra pattern.

[ZEBRA2]

Video level

[ON]

[OFF]

[SPOT]

[109%]

[ZEBRA2 DETECT]

[ZEBRA1 DETECT]

[0%]

To display the zebra pattern in the video of the monitor output terminal (<SDI OUT2>, <VIDEO OUT>, <HDMI OUT>), set in the main menu → [I/F SETUP] → [OUTPUT SEL] → [MONITOR OUT ZEBRA].

Top of the page