- Top
- Preparation
- Mounting and adjusting the lens
- Mounting the lens

# Mounting the lens

Lens lever

Mark

Mount cap

Fig. 1

Fig. 2

Cable clamp

<LENS> terminal

Fig. 4

Fig. 3

Raise the lens lever and remove the mount cap. (Fig. 1)

Align the indentation at the top center of the lens mount with the center mark of the lens to mount the lens. (Fig. 2)

Lower the lens lever to firmly clamp the lens. (Fig. 3)

Secure the cable through the cable clamp and connect it to the <LENS> terminal. (Fig. 4)

Perform lens flange back adjustments.

For details, refer to “Flange back adjustment”.

NOTE

- For handling the lens, refer to the lens operating instructions.

- For details on the current from the <LENS> terminal, refer to “Details of the connector signals”.

- When the lens is removed, install the mount cap to protect the device.

Top of the page