- Top
- Network Connection
- Network function
- Setting for connection with P2 ROP application

# Setting for connection with P2 ROP application

Using the P2 ROP application on an iPad connected to the camera via wireless LAN, you can remotely control some functions.

To connect an iPad to the camera via wireless LAN, configure the settings in the following procedure.

## Network setting on the camera

Set wireless LAN.

Refer to steps 1 to 3 in “[DIRECT] mode” to configure the setting.

Set the remote control function.

Set the main menu → [I/F SETUP] → [USB/LAN] → [NETWORK FUNC] → [HTTP SERVER] to [BROWSE (+CTRL)].

Set the main menu → [I/F SETUP] → [USB/LAN] → [NETWORK FUNC] → [IP REMOTE] to [ENABLE].

Set each item in the main menu → [I/F SETUP] → [USB/LAN] → [NETWORK FUNC] → [USER ACCOUNT].

[USER NAME]: Sets the user account name. (Factory setting: [guest])

[PASSWORD]: Sets the password. (Factory setting: [p2guest]) Enter up to 31 characters for the user account name, and 6 to 15 characters for the password.

## iPad setting

Refer to the help file of P2 ROP application.

NOTE

- To connect an iPad to the camera via wireless LAN, the following information of the camera is required.

  - User account name

  - Password

  - IP address (when the camera’s main menu → [I/F SETUP] → [USB/LAN] → [WIRELESS PROPERTY] → [DHCP SERVER] is set to [ENABLE], IP address does not need to be set)

- When the main menu → [PAINT] → [GAMMA] → [GAMMA MODE SEL] is set to [HLG], the item of [GAMMA] in the [CAM. INFO] panel of the P2 ROP app becomes blank.

Top of the page