- Top
- Network Connection
- Network function
- P2 playlist edit function setting

# P2 playlist edit function setting

## Starting application (P2 Playlist Editor) from web browser

After completing the network connection with your mobile device or computer, start the browser of the mobile device or computer, and then start the application (P2 Playlist Editor).

Fig. 1

Select [ON] in the main menu → [I/F SETUP] → [USB/LAN] → [NETWORK FUNC] → [PLAYLIST].

Changes the mode to the playlist edit mode.

Start the browser of your mobile device or computer (Safari, Internet Explorer).

Enter the IP address set for the camera in the address entry field of the browser.

- Factory setting: [192.168.0.1]

If you use a computer, press the Enter key, and if you use iPad/iPhone, tap the GO button.

The web application (P2 Playlist Editor) starts up.

When the confirmation screen is displayed, enter [USER NAME] and [PASSWORD] on the entry screen.

Enter [USER ACCOUNT] (Factory setting: [guest]) and [PASSWORD] (Factory setting: [p2guest]) that have been set for the camera.

When a screen like (Fig. 1) appears, the connection has been established.

User account name and password can be set in the main menu → [I/F SETUP] → [USB/LAN] → [NETWORK FUNC] → [USER ACCOUNT].

Accounts can be created or deleted, and the passwords can be changed in the main menu → [I/F SETUP] → [USB/LAN] → [NETWORK FUNC] → [ACCOUNT LIST].

Enter up to 31 characters for the user account name, and 6 to 15 characters for the password.

For information on P2 Playlist Editor, refer to the User Guide of “P2 Web Application” on the following website:

https://pro-av.panasonic.net/manual/en/index.html

NOTE

- When [NETWORK SEL] is [OFF] or set to [4G/LTE], the P2 playlist editing function cannot be used.

- The number of clients that can be connected simultaneously during the playlist edit function is 1.

Top of the page