- Top
- Description of Parts
- Audio (output) function section

# Audio (output) function section

1. <MONITOR> (volume adjustment) dial

   Adjust the volume of the speaker and earphones.

2. <ALARM> (alarm volume adjustment) dial

   Adjust the volume of the alarm from the speaker and earphones.

   When set to the minimum position, the alarm cannot be heard.

3. Speaker

   During recording, EE audio can be monitored, and during playback, playback audio can be monitored.

   The alarm is output in sync with flashing/lighting of the <WARNING> lamp or warning indicator.

   Audio from the speaker automatically disappears when earphones are connected to the <PHONES> terminal.

4. Audio channel selector switch

   Switch the audio channels output to the speaker, earphones, and <AUDIO OUT> terminal.

   <CH1/2> | Outputs the signals of audio channels 1 and 2.
   <CH3/4> | Outputs the signals of audio channels 3 and 4.

   The channel display of the audio level meter on the LCD monitor and viewfinder are also switched interlocked to operation of this switch.

5. <MONITOR SELECT> (audio selection) selector switch

   Select audio output from the speaker, earphones and <AUDIO OUT> terminal interlocked with the audio channel selector switch.

   <CH1/3> | Outputs the signal of either audio channel 1 or audio channel 3.
   <ST> | Outputs either the stereo audio signals of audio channels 1 and 2 or the stereo audio signals of audio channels 3 and 4. Stereo audio signals can be changed to the MIX signals in the main menu → [I/F SETUP] → [MIC/AUDIO] → [MONITOR SELECT].
   <CH2/4> | Outputs the signal of either audio channel 2 or audio channel 4.

   <MONITOR SELECT> (audio selection) selector switch | Audio channel selector switch
   --- | ---
   <CH1/2> | <CH3/4>
   <CH1/3> | Audio channel 1 | Audio channel 3
   <ST> | Stereo output from audio channels 1 and 2* | Stereo output from audio channels 3 and 4*
   <CH2/4> | Audio channel 2 | Audio channel 4

   [STEREO] or [MIX] can be switched to in the main menu → [I/F SETUP] → [MIC/AUDIO] → [MONITOR SELECT].

6. <PHONES> (earphones) terminal (mini jack)

   This is the terminal for connecting the audio monitor earphones. (stereo)

   Audio that is output is the same on both terminals (front side, rear side)

7. <AUDIO OUT> terminal

   - Output audio signals recorded on audio channel 1/2 or 3/4.

   - Select output signals by the <MONITOR SELECT> selector switch.

Top of the page