- Top
- Shooting
- Setting the high dynamic range (HDR)
- Recording in high dynamic range (HDR)

# Recording in high dynamic range (HDR)

Select [HLG] in the main menu → [PAINT] → [GAMMA] → [GAMMA MODE SEL].

The output will be as follows.

- <SDI OUT1> terminal: Outputs an image in high dynamic range (hybrid log gamma).

- <SDI OUT2> terminal: Outputs an image in high dynamic range (hybrid log gamma) or standard dynamic range (monitoring gamma) as set in the main menu → [I/F SETUP] → [OUTPUT SEL] → [SDI OUT2 HDR].

- <HDMI OUT> terminal and <VIDEO OUT> terminal: Converts an image as the monitoring gamma for output.

- Viewfinder and LCD monitor: Converts an image as the monitoring gamma for output.

  Press the <USER> button to which [VF/LCD HLG] is assigned to view the image of the hybrid log gamma output temporarily.

NOTE

- Records in BT.709.

- The characters and level of the marker of the <HDMI OUT> terminal become slightly larger and the color of the menu changes slightly.

- [SDI OUT2 HDR] can only be select when main menu → [PAINT] → [GAMMA] → [GAMMA MODE SEL] is set to [HLG].

Top of the page