- Top
- Shooting
- Setting the time data
- Recording and output of time codes and user bits

# Recording and output of time codes and user bits

Recording and output of time codes

[REC FORMAT] indicates only frame rate. For example, [AVC-I100/60i] is 60i, and [AVC-G50/30PN] is 30P.

System setting state | Recording TC | Output TC
--- | --- | ---
[REC FORMAT] | LTC | VITC | TC OUT | LTC, VITC of HD SDI
60P 60i | Recording run/free run*1 [DF]/[NDF] 30 frames | Same value as LTC (No recording in [DV] mode) | LTC is output. | LTC is output. (No recording in [480i] mode)
30P | Recording run/free run*1*2 [DF]/[NDF] 30 frames | Same value as LTC | LTC is output. | LTC is output.
24P | Recording run/free run*3 [NDF] fixed 24 frames | Same value as LTC | LTC is converted to 30 frames and output. | LTC is output.
50P 50i | Recording run/free run*1 25 frames | Same value as LTC (No recording in [DV] mode) | LTC is output. | LTC is output. (No recording in [576i] mode)
25P | Recording run/free run*1*2 25 frames | Same value as LTC | LTC is output. | LTC is output.
24P (when [LINE&FREQ] is [1080-23.98PsF]) | Recording run/free run*4 [NDF] fixed 24 frames | Same value as LTC | LTC is output as 24 frames as is. | LTC is output.

For free run, the time code is slaved to the input TC of the <TC IN> terminal.

Cannot make a slave during recording in native recording mode.

In free run, the time code is converted to 24 frames and slaved when the input TC of the <TC IN> terminal is 30 frame non-drop frame. However, the time code cannot be slaved during recording.

In free run, the time code is slaved when the input TC of the <TC IN> terminal is a non-drop frame. However, the time code cannot be slaved during recording.

Recording and output of user bits

[REC FORMAT] indicates only frame rate. For example, [AVC-I100/60i] is 60i, and [AVC-G50/30PN] is 30P.

System setting state | Recording UB | Output UB
--- | --- | ---
[REC FORMAT] | LTC UB | VITC UB | <TC OUT> terminal UB | LTC UB for HD SDI | VITC UB for HD SDI
60P 60i 50P 50i | Following [UBG MODE]* | Following [VITC UBG MODE] (However, frame information is fixed at [720P]*) | LTC UB is output. | LTC UB is output. (No recording in [480i] and [576i]) | VITC UB is output. (No recording in [480i] and [576i])
30P 24P 25P | Following [UBG MODE].* | Frame information is fixed. | LTC UB is output. | LTC UB is output. | VITC UB is output.

With [EXT], UB of the <TC IN> terminal is slaved.

Top of the page