- Top
- Connecting to External Devices
- Connecting to Remote operation panel (AK-HRP200G)
- Remote control unit connected to the camera

# Remote control unit connected to the camera

When AK-HRP200G is connected to the camera, AK-HRP200G button operations are as follows:

- Matrix button (<MATRIX>), skin tone detail button (<SKINDTL>): Operation varies depending on the lighting status of the button.

  - When the button lights up, the operation is available with the menu setting value of the camera (setting for the linear matrix or skin tone detail).

  - When the button turns off, the function of the linear matrix or skin tone detail is set to [OFF], regardless of the menu setting value.

  After restarting the camera, the menu setting value is reflected in AK-HRP200G.

- Scene/user file switch button <SHIFT>, scene/user file selector button (<SCENE1/USER1> - <SCENE3/USER3>, <SCENE4>): Operation is not available.

- Adjusted value display area (4 digits), display selector button for ND filter/CC filter (<ND/CC>): Zoom and focus are not supported.

- Character/menu button (<CHARA/MENU>): Operation is same as the <MON OUT CHARACTER> switch of the camera.

Top of the page