- Top
- Shooting
- Setting the high dynamic range (HDR)
- Playing back the signal recorded in high dynamic range (HDR)

# Playing back the signal recorded in high dynamic range (HDR)

Detects the recorded information and sets as follows.

#### When recorded information is in high dynamic range

- <SDI OUT1> terminal: Outputs the recorded image directly in high dynamic range (hybrid log gamma).

- <SDI OUT2> terminal: When the main menu → [I/F SETUP] → [OUTPUT SEL] → [SDI OUT2 HDR] is set to [ON], the recorded image is output directly in high dynamic range (hybrid log gamma).

  When the main menu → [I/F SETUP] → [OUTPUT SEL] → [SDI OUT2 HDR] is set to [OFF], the recorded image is converted to standard dynamic range (monitoring gamma) for output.

  When changing the setting of [SDI OUT2 HDR], set main menu → [PAINT] → [GAMMA] → [GAMMA MODE SEL] to [HLG].

- <HDMI OUT> terminal, <VIDEO OUT> terminal, viewfinder and LCD monitor: Converts the recorded image as the monitoring gamma for output.

#### When recorded information is not in high dynamic range or there is no recorded information

- <SDI OUT1> terminal, <SDI OUT2> terminal, <HDMI OUT> terminal, <VIDEO OUT> terminal, viewfinder, LCD monitor: Outputs a recorded image directly.

  The settings in the main menu → [I/F SETUP] → [OUTPUT SEL] → [SDI OUT2 HDR] is disabled.

NOTE

- Outputs in BT.2020 when recorded information is BT.2020.

- Recording information displays only clips recorded in the high dynamic range (hybrid log gamma) in [CAPTURE GAMMA] and [CAPTURE GAMUT] of the main menu → [CLIP] → [PROPERTY] → [VIDEO].

- The characters and the level of the marker output from the <HDMI OUT> terminal become slightly bigger and the color of the menu changes slightly when recorded information is in high dynamic range.

- The <USER> button to which [VF/LCD HLG] is assigned becomes invalid.

Top of the page