- Top
- Playback
- Thumbnail operations
- Reconnecting incomplete clips

# Reconnecting incomplete clips

Incomplete clips may be generated when clips recorded on multiple P2 cards (connected clips) are separately copied from each card. The reconnection function generates one clip (the original, connected clip) from incomplete clips.

Use the cursor buttons and the <SET> button to select incomplete clips to be reconnected.

Usually, thumbnails of incomplete clips (clips with indicator) are displayed in a line.

Select [RE-CONNECT] in the main menu → [CLIP] and press the <SET> button.

Use the cursor buttons and the <SET> button to select [YES].

This reconnects incomplete clips.

NOTE

- Incomplete clip indicators will remain displayed when only some clips are reconnected, unless all the constituent clips of the original clip are reconnected.

Top of the page