- Top
- Maintenance
- Warning system
- Warning information display

# Warning information display

Monitor display | Description | Camera operation
--- | --- | ---
First row | Second row
[AUTH NG CARD] (slot number) | None | CPS authentication of microP2 memory card has failed. The microP2 memory card whose CPS authentication failed cannot be recorded or played back. Select [AUTHENTICATE] in the main menu → [CLIP], and enter the password. For details, refer to “Manual CPS authentication”. | Continue
[BACKUP BATT EMPTY] | None | Displays any reduced voltage detected on the backup battery in the internal clock when the power is turned on. Follow “Charging the built-in battery” to charge the battery. | Continue
[CARD ERROR] (slot number) | None | Displayed when an data error caused by the P2 card occurs during recording. Displayed after recording stops until the next operation. Also displayed for three seconds during playback when a P2 card error causes playback to stop. Replace the P2 card of the slot where the error occurred. | Stop
[CLIP DISCONTINUED] | None | Displayed when clips cannot be linked with the subsequent recording operations due to the inconsistency as linked clips during recording in one-clip recording mode. | Continue
[DIR NG CARD] (slot number) | None | The directory position is not correct. Make a card backup immediately and use again after formatting. | Continue
[FAN STOPPED] | None | Displayed when the fan motor stops. The camera operates even if the fan stops. Refrain from using immediately. | Continue
[PB INTERMITTENT] (slot number) | None | Playback is interrupted on the SDHC/SDXC memory card. A card whose playback performance cannot be assured is inserted. Use of microP2 or P2 memory card is recommended. | Continue
[PROXY ERROR] | None | Proxy error For details, refer to “Error displays about proxy data recordings”. | Continue
[PROXY REC WARNING] | None | Proxy error For details, refer to “Error displays about proxy data recordings”. | Continue
[REC IMPOSSIBLE] (slot number) | None | An SDHC/SDXC memory card is inserted into the microP2 memory card slot. Recording to the SDHC/SDXC memory card is disabled. Record to microP2 or P2 memory cards. | Continue
[REC WARNING] | [FRAME SIGNAL] | Displayed when a video or audio error occurs during recording. Turn the power off and on before using it again. When input signals are disrupted, recording continues while disrupted images are recorded. Check the signal to be input to the camera. | Continue
[REC WARNING] | [OVER MAX# CLIPS] | Displayed when attempting to record in excess of the maximum total number of clips allowed for one P2 card. Replace the P2 card or delete unnecessary clips. It is displayed after approximately 3.5 hours have elapsed from the time when operation to start a single recording is executed when [SHORT SPLIT] is selected in the main menu → [REC/PB] → [REC/PB SETUP] → [FILE SPLIT]. The recording is stopped. | Stop
[REC WARNING] (occurs during recording) | [PULL DOWN] (occurs during recording) [PULL DOWN ERROR] (occurs at times other than during recording) | The video pull-down sequence and time code values are not synchronized. Check the signal. | Continue
[REC WARNING] | [REC DATA] | Displayed when an error occurs in recorded data during recording. Turn the power off and on before using it again. | Continue or Stop
[RUN DOWN CARD] (slot number) | None | The maximum number of overwrites has been exceeded. Replacement of the P2 card is recommended. | Continue
[SD CARD] (slot number) | None | An SDHC/SDXC memory card is inserted into the microP2 memory card slot. The current operation will continue. Use of microP2 or P2 memory card is recommended. | Continue
[SLOT1/2 CANNOT REC] or [SLOT3/4 CANNOT REC] | [microP2 SELECTED] or [P2 SELECTED] | Displayed when the card is inserted into the slot which is not selected as the recording slot. | Stop
[CHECK SLOT] (slot number) | None | The memory card may not be recognized correctly due to reasons such as the microP2 memory card being inserted slowly or dirt on the terminal of the memory card. | Continue Recording cannot be performed on the inserted microP2 memory card. Check the microP2 memory card that is inserted. Insert the microP2 memory card again if this is displayed when the microP2 memory card is inserted.
[TEMPORARY PAUSE] | [IRREGULAR SIG] | Correct recording is not possible due to disruption of input signals of the <GENLOCK IN> or <SDI IN> terminal, and recording is suspended temporarily. The clip will be divided. Recording will be resumed when the signal returns to normal. However, interval recording, one-shot recording, and loop recording will not be resumed. | Suspend → Resume
[WIRELESS-RF] | None | Audio wireless reception status is poor. | Continue
[UP LIST #99/100] | None | The number of registrations in the upload list of the rec during upload function has reached 99. One more clip to the upload list can be registered. Delete unnecessary clips in the upload list. | Continue
[UP LIST #100/100] | None | The number of registrations in the upload list of the rec during upload function has reached the upper limit. When more additional clips need to be registered, delete unnecessary clips in the upload list. | Continue
[UP LIST OVER MAX #] | None | Clips cannot be added for registration because the number of registrations in the upload list of the rec during upload function has reached the upper limit. When additional clips need to be registered, delete unnecessary clips in the upload list. | Continue
[No HDR FLAG] | [at DVCPROHD REC] | Displayed when recording under the following conditions. When the recording format is DVCPRO HD and the main menu → [PAINT] → [GAMMA] → [GAMMA MODE SEL] is set to [HLG] When the recording format is DVCPRO HD, the main menu → [SYSTEM MODE] → [REC SIGNAL] is set to [SDI], and the signal input to the <SDI IN> terminal is in high dynamic range (hybrid log gamma) Recording can be performed even if the message is displayed. However, information indicating the high dynamic range is not recorded to clips. Change the recording format or change the gamma mode to a mode other than the hybrid log gamma to remove the message. | Continue

Top of the page