- Top
- Network Connection
- Network function
- Setting for IP connection with the remote operation panel (AK-HRP200G)

# Setting for IP connection with the remote operation panel (AK-HRP200G)

You can remotely control some functions by connecting the Remote Operation Panel AK-HRP200G (optional) via IP connection.

To connect the AK-HRP200G via wired LAN to remote-control the camera, configure the settings in the following procedure.

Configure the network settings of the AK-HRP200G.

For the network settings, use ROP setup software that is supplied with AK-HRP200G.

Configure the network settings of the camera.

Set the main menu → [I/F SETUP] → [USB/LAN] → [LAN PROPERTY] → [DHCP] to [DISABLE], and refer to steps 1 to 2 in “Wired LAN settings” to configure the network settings.

Set each item in the camera’s main menu → [I/F SETUP] → [USB/LAN] → [NETWORK FUNC] → [USER ACCOUNT].

[USER NAME]: Sets the user account name. (Factory setting: [guest])

[PASSWORD]: Sets the password. (Factory setting: [p2guest])

Enter up to 31 characters for a user account name, and characters between 6 and 15 for a password.

Set the camera’s main menu → [I/F SETUP] → [USB/LAN] → [NETWORK FUNC] → [IP REMOTE] to [ENABLE].

The camera will restart. The IP connection will be possible after the camera is started. The camera will also restart when [IP REMOTE] is set to [DISABLE]. The IP connection mode is canceled after the camera is started.

NOTE

- The following information is required to connect to AK-HRP200G.

  - User account name

  - Password

  - IP address

  - Port number: 49152

- For AK-HRP200G, use Ver.4.01.00 or later versions.

- For details on the operations of ROP setup software, refer to the Operating Instructions of the AK-HRP200G.

- For the ROP setup software, use Ver.3.0.0.0 or later versions.

Top of the page