- Top
- Shooting
- Setting the time data
- User bits settings

# User bits settings

Set LTC UB in the main menu → [REC/PB] → [TC/UB] → [UBG MODE], and set VITC UB in the main menu → [REC/PB] → [TC/UB] → [VITC UBG MODE].

Item name | Description
--- | ---
[USER] (only [UBG MODE]) | Records internal user values. User values can be entered on the status display. Setting values are held even when the power is turned off. For details, refer to “How to input user bits”.
[USER/EXT] (only [VITC UBG MODE]) | Records internal user values as VITC UB. Same value as the user bit that is displayed when [UBG MODE] is set to [USER] or [EXT].
[TIME] | Records the time measured by the internal clock.
[DATE] | Records the hour digit of year/month/day/date-time measured by the internal clock.
[EXT] (only [UBG MODE]) | Records the user bit values currently input to the <TC IN> terminal. User values held internally also change this input value.
[TCG] | Records the time code value.
[FRAME RATE] | Records the camera shooting frame rate information. When playing back clips recorded in native format, the same frame rate information as VITC UB is output regardless of the recorded value. Use the camera at this setting when the editing device such as a computer uses the frame rate information of the user bits.
[REGEN] | Reads the user bit last recorded to P2 card that is currently to be recorded to and recording this value as it is.

Top of the page