- Top
- Shooting
- Setting the time data
- Setting the camera ID

# Setting the camera ID

Set the camera ID in the main menu → [CAMERA] → [CAMERA ID]. Alphanumerics, symbols, and spaces within ten characters can be used.

Fig. 1

Fig. 2

Fig. 3

Select [CAMERA ID] in the main menu → [CAMERA], and use the jog dial button (or cursor buttons /) to navigate to the [ID1] to [ID3] items. (Fig. 1)

Press the jog dial button (or <SET> button).

The camera ID input screen and software keyboard are displayed.

Use the jog dial button (or cursor buttons ///) to select the desired characters. (Fig. 2)

Press the jog dial button (or <SET> button) to apply the character.

Use the jog dial button (or cursor buttons ///) to select [OK], and press the jog dial button (or <SET> button).

The entered character string is set and the screen returns to the selection menu of the camera ID. (Fig. 3)

Press the <MENU> button to end the operation.

NOTE

- While the setting menu is displayed, the camera ID will not be displayed even if the color bar signal is output.

- The following settings can be made in the main menu → [VF] → [VF INDICATOR].

  - When setting [CAMERA ID] to [BAR], the camera ID is recorded at the same time as the color bar signal.

  - The position where the camera ID is superimposed on the color bar can be selected in [ID POSITION].

  - When setting [DATE/TIME] to [ON], date and time information as well as the camera ID can be superimposed on the color bar.

  - When setting [TC ON COLOR BAR] to [ON], the time code is displayed at color bar output. The time code is not recorded.

Top of the page