- Top
- Shooting
- Handling setting data
- Setting data file configuration

# Setting data file configuration

The camera has six file data areas.

Factory data | This area stores factory settings. It cannot be rewritten by menu operation.
User data | This area stores values set by menu operation. As default data, factory data is stored here.
Current data | This area stores the operation status of the camera. Setting values in this area are changed by menu operation.
Scene file | Four scene files are provided.
Lens file | Eight lens files are provided. Eight of these files can be saved together as a single file on SD memory card.
CAC file | This area stores 32 chromatic aberration compensation data.

[CAC FILE (SD CARD)]

SD memory card

Setup data

SD memory card

[LOAD]

CAC file

[SETUP DATA (SD CARD)]

[SETUP DATA (SD CARD)]

Number of files: 32

[LOAD]

[SAVE]

[CAC ADJ.] → [CAC CONTROL]

[SCENE]

Menu operation

Setting valve changed

Scene file

[SAVE]

Current data

Number of files: 4

[SCENE]

(operation status of camera)

[LOAD]

Number of files: 1

[LENS FILE]

Lens file

[LOAD]

Number of files: 8

[LENS FILE]

[INITIALIZE]

[LOAD USER DATA]

[SAVE]

[SAVE USER DATA]

[INITIALIZE]

[LENS FILE (SD CARD)]

[LENS FILE (SD CARD)]

User data

[LOAD]

[SAVE]

Number of files: 1

[LOAD FACTORY DATA]

SD memory card

Factory data

Lens file

(cannot be rewritten)

Number of files: 8×8

Number of files: 1

8 setup files can be written to SD memory card.

: Camera internal files

: Menu operation

NOTE

- For details on items for setup data, user data, and scene file, etc., refer to “Setting items to [USER MENU] and loading/reading the settings to a data file”.

- When recording of a clip by linking to the previous clip is possible in one-clip recording ([1CLIP] is displayed), you cannot operate a scene file or a user file. Close the menu once, press and hold the <STOP> button for approx. 2 seconds to end linking of clips, and then try the operation again. The same applies to interval recording or during standby in one-shot recording.

## Setting up using SD memory cards

An SD memory card (optional) can be used as a setup card that stores setting menu content.

Use of this data allows you to quickly reproduce optimum setup states.

Top of the page