- Top
- Shooting
- Viewfinder status display
- Checking and displaying shooting status

# Checking and displaying shooting status

Each of the display items can be set to display/hide in the setting menu. All display items can be hidden at a time. Also, the mode check [STATUS] screen is displayed when the <MARKER SEL>/<MODE CHECK/MENU CANCEL> switch is pushed towards the <MCK/MCL> side. During mode check, almost all items are displayed including usually hidden items so that the shooting status can be checked. For details on the mode check, refer to “Mode check display”.

No | Display item name | Selection of menu item display/hide | Display status | Display batch off*1 | Mode check display | Display in playback mode
--- | --- | --- | --- | --- | --- | ---
At all times | Relevant menu items only
1 | Shutter speed/mode | [VF INDICATOR] → [SHUTTER] | ✓ | — | ✓ | ✓ | ✓ | —
2 | Camera mode | [VF INDICATOR] → [CAMERA MODE] | ✓ | ✓ | — | ✓ | ✓ | —
3 | HD SDI recording control information | [VF INDICATOR] → [SDI REC STAT] | ✓ | — | ✓ | — | ✓ | —
4 | Proxy information display | [VF INDICATOR] → [PROXY DISP] or [DUAL CODEC SETUP] → [PROXY DISP] | ✓ | — | ✓ | ✓*3 | ✓ | —
5 | SD memory card status display | [VF INDICATOR] → [PROXY DISP] or [DUAL CODEC SETUP] → [PROXY DISP] | ✓ | — | ✓ | ✓*3 | ✓ | —
6 | External GPS status display | [VF INDICATOR] → [EXTERNAL GPS] | ✓ | — | ✓ | ✓ | ✓ | —
7 | Bonding device status display | [VF INDICATOR] → [BONDING DEV.] | ✓ | — | ✓ | ✓ | ✓ | —
4G/LTE connection status display | [VF INDICATOR] → [4G/LTE] | ✓ | — | ✓ | — | ✓ | —
8 | Camera warning, notification display area | [VF DISPLAY] → [DISP MODE] | ✓*4 | — | ✓ | — | ✓ | —
9 | <USER> button assignment information | [VF DISPLAY] → [DISP MODE] | ✓ | — | ✓ | — | ✓ | —
10 | Focus bar display | [VF INDICATOR] → [FOCUS BAR] | ✓ | ✓ | — | ✓ | ✓ | —
11 | Digital zoom ratio display | — | — | — | ✓ | ✓ | ✓ | —
12 | Extender | [VF INDICATOR] → [EXTENDER] | ✓ | — | ✓ | ✓ | ✓ | —
13 | Color temperature | [VF INDICATOR] → [COLOR TEMP] | ✓ | ✓ | — | ✓ | ✓ | —
14 | Filter position | [VF INDICATOR] → [FILTER] | ✓ | ✓ | — | ✓ | ✓ | —
15 | <WHITE BAL> switch position | [VF INDICATOR] → [WHITE] | ✓ | ✓ | — | ✓ | ✓ | —
16 | Dynamic range stretcher (DRS) function display | [VF INDICATOR] → [DRS] | ✓ | — | ✓ | ✓ | ✓ | —
17 | Incremental gain display | [VF INDICATOR] → [GAIN] | ✓ | — | ✓ | ✓ | ✓ | —
18 | Gain display | [VF INDICATOR] → [GAIN] | ✓ | ✓ | — | ✓ | ✓ | —
19 | System information and warning | [VF INDICATOR] → [SYSTEM INFO] | ✓ | — | ✓ | — | ✓ | ✓
20 | Time code display | [VF INDICATOR] → [TC] | ✓ | ✓ | — | ✓ | ✓ | ✓
21 | Audio input line and level meter display | [VF INDICATOR] → [AUDIO LVL] | ✓ | ✓ | — | ✓ | ✓*5 | —
22 | Iris override display | [VF INDICATOR] → [IRIS] | ✓ | — | ✓ | ✓ | ✓ | —
23 | Super iris display | [VF INDICATOR] → [IRIS] | ✓ | — | ✓ | ✓ | ✓ | —
24 | Iris, F value | [VF INDICATOR] → [IRIS] | ✓ | ✓*6 | — | ✓ | ✓ | —
25 | Super black display | [VF INDICATOR] → [IRIS] | ✓ | — | ✓ | ✓ | ✓ | —
26 | Zoom display | [VF INDICATOR] → [ZOOM/FOCUS] | ✓ | ✓*6 | — | ✓ | ✓ | —
27 | Focus information display | [VF INDICATOR] → [ZOOM/FOCUS] | ✓ | ✓*6 | — | ✓ | ✓ | —
28 | Information display such as interval recording/pre-recording | [VF INDICATOR] → [P-REC/i-REC] | ✓ | — | ✓ | — | ✓ | —
29 | Gamma mode display | [VF INDICATOR] → [GAMMA MODE] | ✓ | ✓ | — | ✓ | ✓ | —
30 | Lock status display of auto tracking white balance | [VF INDICATOR] → [WHITE] | ✓ | — | ✓ | ✓ | ✓ | —
31 | Type of marker | [VF DISPLAY] → [DISP MODE] | ✓ | — | ✓ | — | ✓ | —
32 | Network information display | — | — | — | — | — | ✓ | —
33 | Streaming setting status display | — | — | — | — | — | ✓ | —
34 | Y GET brightness display | — | — | — | ✓ | ✓ | ✓ | —
35 | Remote control display in an IP connection | — | — | — | — | — | ✓ | —
36 | Compression mode | [VF INDICATOR] → [COMPRESSION] | ✓ | — | ✓ | ✓ | ✓ | —
37 | High-sensitivity mode display | [VF INDICATOR] → [SHOOTING MODE] | ✓ | — | ✓ | ✓ | ✓ | —
38 | Flash band compensation (FBC) function display | [VF INDICATOR] → [FBC] | ✓ | — | ✓ | ✓ | ✓ | —
39 | Chromatic aberration compensation | [VF INDICATOR] → [CAC] | ✓ | — | ✓ | ✓ | ✓ | —
40 | Battery charge level/voltage | [VF INDICATOR] → [BATTERY] | ✓ | ✓ | — | ✓*3 | ✓ | —
41 | P2 card remaining free space | [VF INDICATOR] → [P2CARD REMAIN] | ✓*2 | ✓ | — | ✓*2 | ✓ | —
42 | Simultaneous recording mode display | [VF INDICATOR] → [P-REC/i-REC] | ✓ | — | ✓ | ✓ | ✓ | —
43 | Recording media display | [VF INDICATOR] → [REC MEDIA] | ✓ | ✓ | — | ✓ | ✓ | —
44 | Rec during upload function status display | [VF INDICATOR] → [REC DURING UPLOAD] | ✓ | — | ✓ | ✓ | ✓ | ✓
45 | Recording operation status display | [VF INDICATOR] → [REC STATUS] or [REC/PB SETUP] → [REC TALLY] | ✓ | — | ✓ | — | ✓ | —
46 | Streaming distribution status display | [VF INDICATOR] → [STREAMING] | ✓ | — | ✓ | ✓ | ✓ | —
47 | Recording format | [VF INDICATOR] → [REC FORMAT] | ✓ | ✓ | — | ✓ | ✓ | —
48 | System mode | [VF INDICATOR] → [SYSTEM MODE] | ✓ | ✓ | — | ✓ | ✓ | —

Set in the main menu → [VF] → [VF DISPLAY] → [DISP CONDITION].

Warnings and display during changes cannot be turned off.

Warning cannot be turned off.

Partially displayed.

Displays the input information of all four channels.

Not displayed when there is no information.

Top of the page