- Top
- Shooting
- Setting the electronic shutter
- Setting the synchro scan mode

# Setting the synchro scan mode

Follow the steps below to operate.

<SHUTTER> switch

<SYNCHRO SCAN> adjustment button

Press the <SHUTTER> switch from the <ON> side towards the <SEL> side to set the camera to synchro scan mode.

Operate the <SYNCHRO SCAN> adjustment button to switch the mode continuously.

The shutter speed display in the synchro scan mode can be switched between seconds and angle in the main menu → [VF] → [VF DISPLAY] → [SYNCHRO SCAN DISP].

Top of the page