- Top
- Preparation
- P2 card
- Preventing accidental erasure

# Preventing accidental erasure

To prevent the content of a P2 card from being accidentally erased, set the write-protect switch on the P2 card to the Protect (or LOCK) position.

Write-protect switch

Write-protect switch

NOTE

- Write-protect switch can be switched while the card is being accessed (during recording or playback), but does not take effect until accessing of the card stops.

Top of the page