- Top
- Preparation
- Power supply
- Using external DC power supply

# Using external DC power supply

DC cable

External DC power supply

<DC IN> terminal

Connect the external DC power supply to the <DC IN> terminal of the camera.

Turn on the power switch of the external DC power supply (if the external DC power supply has a power switch).

Turn the <POWER> switch of the camera to < > (ON).

#### External DC power supply Connect after making sure that the output voltage of the external DC power supply is compatible with the rated voltage of the camera. Select an output amperage for the external DC power supply with a margin above the total amperage of the connected devices. The total amperage of connected devices can be calculated with the following formula. Total power consumption ÷ Voltage When the power of the camera is turned on, inrush current is generated. Insufficient power supply when turning on the power may cause a malfunction. We recommend that you use an external DC power supply that can assure double the capacity of the total power consumption of the camera and connected devices that are turned on by interlock when the power of the camera is turned on (such as lenses, wireless microphone receivers). For the DC cable, use a dual-core shielded wire of AWG18 (nominal cross section area 0.824 mm2) or thicker.

Make sure of the pin alignment of the DC output terminal of the external DC power supply and the camera <DC IN> terminal, and connect the polarity correctly. If the +12 V power supply is connected to the GND terminal in error, it may cause fire or malfunction.

DC IN
| 1 | GND
2 | NC
3 | NC
4 | +12 V
Panasonic Part No.: K1AA104H0038 Manufacturer Parts No.: HA16RX-4P (SW1) (76) (Hirose Electric Co.)

NOTE

- When both the battery and the external DC power supply are connected, the power supply from the external DC power supply has priority. The battery may be removed while using the external DC power supply.

- When using an external DC power supply, always turn the power switch of the external DC power supply on before turning the <POWER> switch of the camera to < > (ON). If the operations are performed in reverse, the camera may malfunction because the external DC power supply output voltage rises too slowly.

- When power is supplied from the <DC IN> terminal, the light circuit does not function. The light circuit can be used only when power is supplied from the Anton/Bauer battery plate.

- When connecting the battery to the <DC IN> terminal, set the battery type in the main menu → [I/F SETUP] → [BATTERY/P2CARD] → [EXT DC IN SELECT]. However, in that case, % display is not possible for batteries with a battery level indicator function.

Top of the page