- Top
- Shooting
- Multi formats
- List of recording settings and recording functions

# List of recording settings and recording functions

The recording modes of the camera act as follows depending on the setting of [REC SIGNAL] in the main menu → [SYSTEM] → [SYSTEM MODE] and the setting of [RECORDING] in [REC/PB] → [REC FUNCTION]. Even in “Available” cases, recording functions are restricted in some system modes. For details, refer to the table in “System modes and recording functions”.

Setting | Recording setting (setting menu) | Recording/operation enabled/disabled
--- | --- | ---
Operation mode | [REC SIGNAL] | [REC FUNCTION] | Pre-recording | One-clip recording | Simultaneous recording
Interval recording | [CAM] | [INTERVAL] | Not available | Not available | Not available
One-shot recording | [CAM] | [ONE SHOT] | Not available | Not available | Not available
Loop recording | [CAM] | [LOOP] | Not available | Not available | Not available
Standard recording | [CAM] | [NORMAL] | Available | Available | Available
SDI input recording | [SDI] | Disabled | Not available | Not available | Available

Setting | Recording setting (setting menu) | Recording/operation enabled/disabled
--- | --- | ---
Operation mode | [REC SIGNAL] | [REC FUNCTION] | Dual codec recording | Text memo | Shot mark
Interval recording | [CAM] | [INTERVAL] | Not available | Not available | Not available
One-shot recording | [CAM] | [ONE SHOT] | Not available | Not available | Not available
Loop recording | [CAM] | [LOOP] | Not available | Not available | Not available
Standard recording | [CAM] | [NORMAL] | Available | Available | Available
SDI input recording | [SDI] | Disabled | Available* | Available | Available

It is not available when [LINE&FREQ] is [480-59.94i] or [576-50i].

Top of the page