- Top
- Network Connection
- Network function
- Connection settings for the streaming function

# Connection settings for the streaming function

You can perform live streaming of audio and video from the camera over the network (wired LAN, wireless LAN, 4G/LTE).

Streaming can be performed through an application software (e.g. P2 Browser, P2 Streaming Receiver) of a device connected to the camera through a network, or through a server that is capable of receiving streaming video sent from the camera.

There are two ways to start streaming: streaming from an application software and streaming from the camera. This section describes the camera's network connection method for each method.

For the procedures on using the streaming function, refer to “Using the streaming function”.

NOTE

- To display the streaming video in the P2 Browser, start the streaming distribution by operation from the application software. The streaming video cannot be displayed when operated from the camera.

## Setting when starting streaming through operation from an application software

Set the connection method when connecting the camera to a network.

Select [WLAN], [4G/LTE], or [LAN] in main menu → [I/F SETUP] → [USB/LAN] → [NETWORK SEL]. For details on each connection method, refer to “Wireless LAN settings” and “Wired LAN settings”.

NOTE

- [4G/LTE] is disabled when connecting to the P2 Browser.

## Setting when starting streaming through operation from the camera

There are two ways to configure the network settings on the camera: configuring the settings from the camera menu or using the settings contained in the SD memory card.

### Configuring the settings from the camera

The followings are the steps to configure the settings from the camera menu.

Set the connection method when connecting the camera to a network.

Select [WLAN], [4G/LTE], or [LAN] in main menu → [I/F SETUP] → [USB/LAN] → [NETWORK SEL]. For details on each connection method, refer to “Wireless LAN settings” and “Wired LAN settings”.

Configure the network settings of the camera.

Select [INTERNAL] in main menu → [I/F SETUP] → [USB/LAN] → [STREAMING SETTING] → [SETTING DATA].

Set each item by matching the connection destinations in main menu → [I/F SETUP] → [USB/LAN] → [STREAMING SETTING].

[SERVER ADDR.]: Sets the IP address of the connection destination.

[RTSP PORT]: Set the RTSP port number of the destination.

NOTE

- You can save the details you have set in Step 2 to an SD through the following procedure: Insert the SD memory card and select [SAVE (SD CARD)] in main menu → [I/F SETUP] → [USB/LAN] → [STREAMING SETTING].

### Configuring the settings by directly referring to the settings contained in the SD memory card

Configure the settings by directly referring to the settings contained in the SD memory card without saving it in the camera.

First, insert the SD memory card that contains the settings, then turn on the power of the camera.

Set the connection method when connecting the camera to a network.

Select [WLAN], [4G/LTE], or [LAN] in main menu → [I/F SETUP] → [USB/LAN] → [NETWORK SEL]. For details on each connection method, refer to “Wireless LAN settings” and “Wired LAN settings”.

Configure the network settings of the camera.

Select [SD CARD] in main menu → [I/F SETUP] → [USB/LAN] → [STREAMING SETTING] → [SETTING DATA].

NOTE

- The setting value of the SD memory card can be saved in following method.

  - Select [SAVE (SD CARD)] in the main menu → [I/F SETUP] → [USB/LAN] → [STREAMING SETTING].

### Configuring the settings after saving the settings contained in the SD memory card to the camera

Configure the settings after saving the settings contained in the SD memory card to the camera.

Set the connection method when connecting the camera to a network.

Select [WLAN], [4G/LTE], or [LAN] in main menu → [I/F SETUP] → [USB/LAN] → [NETWORK SEL]. For details on each connection method, refer to “Wireless LAN settings” and “Wired LAN settings”.

Configure the network settings of the camera.

Select [INTERNAL] in the main menu → [I/F SETUP] → [USB/LAN] → [STREAMING SETTING] → [SETTING DATA].

Insert the SD memory card which contains the settings and select [LOAD (SD CARD)] in main menu → [I/F SETUP] → [USB/LAN] → [STREAMING SETTING].

Top of the page