- Top
- Overview
- Use of the camera on a system
- Basic configuration devices

# Basic configuration devices

Lenses, batteries, etc. are needed for shooting with the camera.

Part name | Part No. | Remark
--- | --- | ---
Electronic HD color view finder | AG-CVF15G/AJ-CVF50G | “Adjusting and setting the viewfinder”
Super-directional electret stereo microphone (phantom +48V) | AJ-MC900G | “Using the front microphone”
Lens (Bayonet type) | FUJINON/CANON | “Mounting and adjusting the lens”
Battery | HYTRON140*1 DIONIC HC/90*1 V-mount type battery plate ENDURA E-10 | “Mounting and setting battery”
SD memory card*2 P2 memory card*2 microP2 memory card*2 | Visit the support desk at the website*2. | “P2 card”
microP2 card adaptor | AJ-P2AD1G | “P2 card”

A battery holder is provided as standard on the main unit.

For the latest information on P2 cards and SD memory cards that are not described in the Operating Instructions, visit the support desk at the following website:

https://pro-av.panasonic.net/

Top of the page