- Top
- Network Connection
- Rec during upload function

# Rec during upload function

Clips recorded in the P2 card can be automatically transferred to a server device on the network during recording/playback with the camera.

The rec during upload function has the following two modes:

- Automatic transfer mode: After the rec during upload function is enabled, uploads recorded clips in order.

- Manual selection mode: Uploads clips selected beforehand.

To use the rec during upload function, network settings and FTP client settings need to be configured beforehand.

The rec during upload function can also be set in [OPTION MENU] → [NETWORK MODE] → [FTP MODE].

Transferring recorded clips automatically (automatic transfer mode)
Transferring selected clips automatically (manual selection mode)
Displaying the upload list
Top of the page