- Top
- Specification
- Dimensions/specifications
- Specifications

# Specifications

## General

Power DC 12 V (11.0 V – 17.0 V) Power consumption 29 W (body only, 1080/59.94i, AVC-Intra 100 standard recording status, LCD ON) 70 W (with all optional accessories connected and maximum power supplied from each output terminal)

indicates safety items.

Ambient operating temperature | 0 °C – 40 °C (32 °F – 104 °F)
Ambient operating humidity | 10% – 85% (relative humidity)
Storage temperature | −20 °C – 60 °C (−4 °F – 140 °F)
Weight | Approx. 3.4 kg (7.5 lbs.) (body only, excluding battery and accessories)
Dimensions (W×H×D) | Body only 147 mm×267 mm×342 mm (5-25/32 inches×10-1/2 inches×13-15/32 inches) (excluding protrusion)

## Camera unit

Pickup device | 2/3-type 2.2 million pixels, MOS×3
Lens mount | 2/3-type bayonet
Optical filter | CC filter | A: 3200 K, B: 4300 K, C: 5600 K, D: 6300 K
ND filter | 1: CLEAR, 2: 1/4ND, 3: 1/16ND, 4: 1/64ND
Gain setting | [NORMAL] mode | −3 dB, 0 dB, 3 dB, 6 dB, 9 dB, 12 dB, 15 dB, 18 dB, 21 dB, 24 dB, 27 dB, 30 dB
[HIGH SENS.] mode | −6 dB, −3 dB, 0 dB, 3 dB, 6 dB, 9 dB, 12 dB, 15 dB, 18 dB, 21 dB, 24 dB, 27 dB, 30 dB
Digital super gain (DS.GAIN) | Selectable from 6 dB, 10 dB, 12 dB, 15 dB, 20 dB, 24 dB, 28 dB, 34 dB
Super gain (S.GAIN) | Selectable from 30 dB, 36 dB, 42 dB
Shutter speed | When [SYSTEM MODE] = 59.94 Hz
60i/60p/30p/24p mode | 1/100 sec., 1/120 sec., 1/250 sec., 1/500 sec., 1/1000 sec., 1/2000 sec., HALF
180.0 deg, 172.8 deg, 144.0 deg, 120.0 deg, 90.0 deg, 45.0 deg
When [SYSTEM MODE] = 50 Hz
50i/50p/25p mode | 1/60 sec., 1/120 sec., 1/250 sec., 1/500 sec., 1/1000 sec., 1/2000 sec., HALF
180.0 deg, 172.8 deg, 144.0 deg, 120.0 deg, 90.0 deg, 45.0 deg
Synchro scan shutter | 1/60.1 sec. – 1/7200 sec. (60i/60p mode)
1/30.0 sec. – 1/3600 sec. (30p mode)
1/24.0 sec. – 1/2880 sec. (24p mode)
1/50.1 sec. – 1/6000 sec. (50i/50p mode)
1/25.0 sec. – 1/3000 sec. (25p mode)
Shutter open angle | Configurable between 3 deg and 359.5 deg (in 0.5 deg steps)
Sensitivity | [NORMAL] mode | F9 (2000 lx, 3200 K, 89.9% reflection, 1080/59.94i) F10 (2000 lx, 3200 K, 89.9% reflection, 1080/50i)
[HIGH SENS.] mode | F12 (2000 lx, 3200 K, 89.9% reflection, 1080/59.94i) F13 (2000 lx, 3200 K, 89.9% reflection, 1080/50i)
Minimum subject illumination | Approx. 0.004 lx (F1.4, +42 dB (S.GAIN), +34 dB (DS.GAIN))
Image S/N | 62 dB (standard)
Horizontal resolution | 1000 TV or higher (center)

## Memory card recorder

Recording media | P2 memory card, microP2 memory card
System format | 1080/59.94p, 1080/59.94i, 1080/23.98PsF, 720/59.94p, 480/59.94i 1080/50p, 1080/50i, 720/50p, 576/50i
Recording format | AVC-Intra 200/AVC-Intra 100/AVC-Intra 50 AVC-LongG 50/AVC-LongG 25/AVC-LongG 12 Switching DVCPRO HD/DVCPRO50/DVCPRO/DV formats
Recording video signal | 1080/59.94p, 1080/29.97pN, 1080/23.98pN, 1080/59.94i 720/59.94p, 720/29.97pN, 720/23.98pN, 480/59.94i 1080/50p, 1080/25pN, 1080/50i 720/50p, 720/25pN, 576/50i
Recording and playback time | AVC-Intra 200 | 64 GB×1 approx. 32 min
AVC-Intra 100/DVCPRO HD | 64 GB×1 approx. 64 min
AVC-Intra 50/AVC-LongG 50/DVCPRO50 | 64 GB×1 approx. 128 min
AVC-LongG 25/DVCPRO/DV | 64 GB×1 approx. 256 min
AVC-LongG 12 | 64 GB×1 approx. 480 min
Figures are for continuous recording as one clip. Depending on the number of clips, the overall recording time may be shorter than the above.

## Digital video

Sampling frequency | AVC-Intra 200/AVC-Intra 100/AVC-LongG 50/AVC-LongG 25/AVC-LongG 12/DVCPRO HD | Y: 74.1758 MHz, PB/PR: 37.0879 MHz (59.94 Hz) Y: 74.2500 MHz, PB/PR: 37.1250 MHz (50 Hz)
DVCPRO50 | Y: 13.5 MHz, PB/PR: 6.75 MHz
DVCPRO | Y: 13.5 MHz, PB/PR: 3.375 MHz
Quantizing | AVC-Intra 200/AVC-Intra 100/AVC-Intra 50/AVC-LongG 50/AVC-LongG 25: 10 bits
AVC-LongG 12/DVCPRO HD/DVCPRO50/DVCPRO/DV: 8 bits
Video compression format | AVC-Intra 200/AVC-Intra 100/AVC-Intra 50 | MPEG-4 AVC/H.264 Intra Profile
AVC-LongG 50/AVC-LongG 25/AVC-LongG 12 | MPEG-4 AVC/H.264
DVCPRO HD/DVCPRO50/ DVCPRO | DV-Based Compression
DV | DV Compression

## Digital audio

Recording audio signal | AVC-Intra 200 | 48 kHz/24 bits, 4CH
AVC-Intra 100/AVC-Intra 50 | 48 kHz/16 bits, 4CH and 48 kHz/24 bits, 4CH switch
AVC-LongG 50/AVC-LongG 25 | 48 kHz/24 bits, 4CH
AVC-LongG 12/DVCPRO HD/DVCPRO50/DVCPRO/DV | 48 kHz/16 bits, 4CH
Headroom | 18 dB/20 dB switchable menu

## Proxy

Video compression format | MPEG4 Simple Profile H.264/AVC Baseline Profile H.264/AVC High Profile
Audio compression format | AAC-LC Linear PCM
Approximate recording time (1 GB) | AVC-G6 2CH MOV | Approx. 13 min
STD 2CH MP4 | Approx. 78 min
SHQ 2CH MOV | Approx. 25 min
HQ 2CH MOV | Approx. 78 min
HQ 4CH MOV | Approx. 72 min
LOW 2CH MOV | Approx. 135 min
These are reference values for continuous recording using the Panasonic products. The recording time may differ depending on the scene or the number of clips.

## Video input/output

<SDI IN> terminal | BNC×1
HD (3G/1.5G), SD: 0.8 V [p-p], 75 Ω
Switch the menu to use as <SDI IN> terminal/return video input terminal/<GENLOCK IN> terminal
<SDI OUT1> terminal | BNC×1
HD (3G/1.5G), SD: 0.8 V [p-p], 75 Ω
<SDI OUT2> terminal | BNC×1
HD (3G/1.5G), SD: 0.8 V [p-p], 75 Ω
<VIDEO OUT> terminal | BNC×1
Composite | 1.0 V [p-p], 75 Ω
<HDMI OUT> terminal | HDMI×1 (HDMI type A terminal, not compatible with VIERA Link)

## Audio input/output

<AUDIO IN> terminal <CH1>/<CH2> | XLR×2, 3-pin <LINE>/<MIC>/<MIC+48V> switchable type
<LINE> | 4 dBu (−3 dBu/0 dBu/4 dBu selectable menu)
<MIC> | −60 dBu (−60 dBu/−50 dBu selectable menu)
<MIC+48V> | Phantom +48 V supported, −60 dBu (−60 dBu/−50 dBu selectable menu)
<MIC IN> terminal | XLR×1, 5-pin Phantom +48 V (selectable menu), −40 dBu (−50 dBu/−40 dBu selectable menu)
Wireless slot | 25-pin, D-SUB, −40 dBu, 2ch supported
<AUDIO OUT> terminal <CH1>/<CH2> | XLR×1, 5-pin
+4 dBu (−3 dBu/0 dBu/4 dBu selectable menu), equilibrium low impedance
<PHONES> terminal | Stereo mini jack × 2 (output impedance 100 Ω)
Speaker | 20 mm diameter, round×1

## Other input/output

<GENLOCK IN> terminal | BNC×1, 1.0 V [p-p], 75 Ω
<TC IN> terminal | BNC×1, 0.5 V [p-p] – 8 V [p-p], 10 kΩ
<TC OUT> terminal | BNC×1, 2.0 ± 0.5 V [p-p], low impedance
<DC IN> terminal | XLR×1, 4-pin, DC 12 V (DC 11.0 V – 17.0 V)
<DC OUT> terminal | 4-pin, DC 12 V (DC 11.0 V – 17.0 V), maximum output current 1.5 A
<REMOTE> terminal | 10-pin
<LENS> terminal | 12-pin
<VF> terminal | 20-pin
<LAN> terminal | 100BASE-TX/10BASE-T
<USB2.0> terminal (device) | Type B connector, 4-pin
<USB3.0> terminal (host) | Type A connector, 9-pin
<USB2.0> terminal (host) | Type A connector, 4-pin
<LIGHT> terminal | 2-pin, DC 12 V (DC 11.0 V – 17.0 V), maximum output current 4.5 A (up to 50 W equivalent)
LCD monitor | 3.5-inch QHD color monitor, approx. 1560000 dots

Top of the page