- Top
- Shooting
- Dual codec recording
- Checking the proxy data

# Checking the proxy data

- The indicator is displayed for the material clips with the proxy data recorded.

- The detailed information of the recorded proxy data can be viewed in the clip property.

  For details on operations, refer to “Checking detailed information of the proxy data”.

- The proxy data is recorded to the P2 card or SD memory card as a video/audio file and real-time metadata file.

  - Video/audio file:XXXXXXXX.MP4 or XXXXXXXX.MOV

  - Real-time metadata file:XXXXXXXX.BIN

    The time code, user bits, and information are recorded to the frame unit.

  Use P2 Viewer Plus to check the proxy data. Some versions of P2 Viewer Plus may not be able to check the data.

  For information on P2 Viewer Plus, visit the following website:

  https://pro-av.panasonic.net/

NOTE

- Clips with proxy data recorded with the camera are handled as unknown clips by some P2 devices. (unknown clip indicator) is displayed on the thumbnail, and the following operations become unavailable. (Except in [STD 2CH MP4] mode)

  - [DELETE]

  - [REPAIR CLIP]

  - [RE-CONNECTION]

  - [COPY]

  - [EXCH. THUMBNAIL]

  - Adding and deleting [TEXT MEMO] and [SHOT MARK]

  Playback is possible.

  On these devices, individual clips with proxy data combined from multiple clips are displayed as an incomplete clip . (Except in [STD 2CH MP4] mode)

## Checking detailed information of the proxy data

Operation methods and panels may differ by version.

Press the <THUMBNAIL> button.

The thumbnail screen appears on the viewfinder screen.

Select [CLIP PROPERTY] in the main menu → [CLIP] → [PROPERTY].

The clip property screen is displayed.

Use the cursor buttons to select [PROXY].

Press the <SET> button.

Detailed information about the proxy data is displayed as below.

#### Detailed information about proxy data

[FORMAT] | The file format of the recorded data is displayed.
[VIDEO CODEC] | Video codec information of the recorded data is displayed.
[VIDEO FRAME RATE] | Video frame rate information of the recorded data is displayed.
[VIDEO BIT RATE] | Video bitrate information of the recorded data is displayed.
[VIDEO RESOLUTION] | The video resolution of the recorded data is displayed.
[ASPECT RATIO] | The aspect ratio of the recorded data is displayed.
[TC SUPER] | An indication whether the TC (time code) display is superimposed over the recorded video.
[AUDIO CODEC] | Audio codec information of the recorded data is displayed.
[AUDIO BIT RATE] | Audio bitrate information of the recorded data is displayed.
[AUDIO SAMPLING RATE] | Audio sampling rate information of the recorded data is displayed.
[NUM.OF AUDIO CH] | The number of audio channels of the recorded data is displayed.

Top of the page