- Top
- Menu Operations
- Menu list
- [PAINT]

# [PAINT]

These are items for performing fine image adjustments while monitoring the output waveform of the camera using the waveform monitor. You will need support from video engineers to use configure these settings.

These menu item settings are enabled when using the camera as a standalone device.

These menu items can be set from an external remote controller.

These menu items cannot be set when the thumbnail screen is displayed.

## [RB GAIN CONTROL]

Item | Description of settings
--- | ---
[R GAIN AWB PRE] | Sets the Rch gain when the <WHITE BAL> switch is on <PRST>. [−200]…[200] Factory setting: [0]
[B GAIN AWB PRE] | Sets the Bch gain when the <WHITE BAL> switch is on <PRST>. [−200]…[200] Factory setting: [0]
[R GAIN AWB A] | Sets the Rch gain when the <WHITE BAL> switch is on <A>. [−200]…[200] Factory setting: [0]
[B GAIN AWB A] | Sets the Bch gain when the <WHITE BAL> switch is on <A>. [−200]…[200] Factory setting: [0]
[R GAIN AWB B] | Sets the Rch gain when the <WHITE BAL> switch is on <B>. [−200]…[200] Factory setting: [0]
[B GAIN AWB B] | Sets the Bch gain when the <WHITE BAL> switch is on <B>. [−200]…[200] Factory setting: [0]
[AWB A GAIN OFFSET] | Sets the Rch gain and Bch gain when performing automatic white balance after the <WHITE BAL> switch is on <A>. [ON]: Keeps the values set in [R GAIN AWB A] and [B GAIN AWB A]. [OFF]: Sets the value of Rch gain and Bch gain to [0]. Factory setting: [OFF]
[AWB B GAIN OFFSET] | Sets the Rch gain and Bch gain when performing automatic white balance after the <WHITE BAL> switch is on <B>. [ON]: Keeps the values set in [R GAIN AWB B] and [B GAIN AWB B]. [OFF]: Sets the value of Rch gain and Bch gain to [0]. Factory setting: [OFF]

NOTE

- Settings made through the menu are disabled when the remote control unit and extension control unit are connected. (Setting values are displayed.)

## [RGB BLACK CONTROL]

Item | Description of settings
--- | ---
[MASTER PED] | Sets the master pedestal level. [−200]…[200] Factory setting: [16]
[R PEDESTAL] | Sets the Rch pedestal level. [−100]…[100] Factory setting: [0]
[G PEDESTAL] | Sets the Gch pedestal level. [−100]…[100] Factory setting: [0]
[B PEDESTAL] | Sets the Bch pedestal level. [−100]…[100] Factory setting: [0]
[PEDESTAL OFFSET] | Sets the Rch, Gch, and Bch pedestal levels after adjusting the automatic black balance. [ON]: Keeps each of the values set in [R PEDESTAL], [G PEDESTAL], and [B PEDESTAL]. [OFF]: Sets the pedestal level of Rch, Gch, and Bch to [0]. Factory setting: [OFF]
[R FLARE] | Adjusts the Rch flare level. The adjusted value of this item is added to the flare adjusted value in the main menu → [MAINTENANCE] → [LENS FILE ADJ.]. [−100]…[100] Factory setting: [0]
[G FLARE] | Adjusts the Gch flare level. The adjusted value of this item is added to the flare adjusted value in the main menu → [MAINTENANCE] → [LENS FILE ADJ.]. [−100]…[100] Factory setting: [0]
[B FLARE] | Adjusts the Bch flare level. The adjusted value of this item is added to the flare adjusted value in the main menu → [MAINTENANCE] → [LENS FILE ADJ.]. [−100]…[100] Factory setting: [0]

NOTE

- Settings made through the menu are disabled when the remote control unit and extension control unit are connected. (Setting values are displayed.)

## [MATRIX]

Item | Description of settings
--- | ---
[[S] L MATRIX TABLE] | Selects the color correction table when the <GAIN> switch is on <L>. [A], [B], [OFF] Factory setting: [A]
[[S] M MATRIX TABLE] | Selects the color correction table when the <GAIN> switch is on <M>. [A], [B], [OFF] Factory setting: [A]
[[S] H MATRIX TABLE] | Selects the color correction table when the <GAIN> switch is on <H>. [A], [B], [OFF] Factory setting: [A]
[[S] MATRIX TABLE] | Selects the color collection table for the linear matrix. [A], [B] Factory setting: [A]
[MATRIX R-G] | Adjusts the linear matrix. (Red - Green) [A]: [−63]…[63] Factory setting: [30] [B]: [−63]…[63] Factory setting: [24]
[MATRIX R-B] | Adjusts the linear matrix. (Red - Blue) [A]: [−63]…[63] Factory setting: [−5] [B]: [−63]…[63] Factory setting: [10]
[MATRIX G-R] | Adjusts the linear matrix. (Green - Red) [A]: [−63]…[63] Factory setting: [−1] [B]: [−63]…[63] Factory setting: [4]
[MATRIX G-B] | Adjusts the linear matrix. (Green - Blue) [A]: [−63]…[63] Factory setting: [3] [B]: [−63]…[63] Factory setting: [12]
[MATRIX B-R] | Adjusts the linear matrix. (Blue - Red) [A]: [−63]…[63] Factory setting: [−1] [B]: [−63]…[63] Factory setting: [5]
[MATRIX B-G] | Adjusts the linear matrix. (Blue - Green) [A]: [−63]…[63] Factory setting: [2] [B]: [−63]…[63] Factory setting: [20]

NOTE

- When saving or reading setup files from an SD memory card, you can save items with an [S] and items without an [S] separately. Items with an [S] in front of the item name are the targets for [PAINT([S]SELECT)] in the main menu → [FILE] → [SETUP DATA SELECT]. Items without an [S] are targets for [PAINT(LEVEL)].

## [COLOR CORRECTION]

Item | Description of settings
--- | ---
[[S] L COLOR CORRECT] | Switches [ON]/[OFF] of the 15-axis independent color correction where the <GAIN> switch is on <L>. [ON], [OFF] Factory setting: [ON]
[[S] M COLOR CORRECT] | Switches [ON]/[OFF] of the 15-axis independent color correction where the <GAIN> switch is on <M>. [ON], [OFF] Factory setting: [ON]
[[S] H COLOR CORRECT] | Switches [ON]/[OFF] of the 15-axis independent color correction where the <GAIN> switch is on <H>. [ON], [OFF] Factory setting: [ON]
[R (SAT)] | Corrects red color saturation. [−63]…[63] Factory setting: [34]
[R-R-Mg (SAT)] | Corrects the color saturation between red and “colors between red and magenta”. [−63]…[63] Factory setting: [22]
[R-Mg (SAT)] | Corrects the color saturation between red and magenta. [−63]…[63] Factory setting: [20]
[Mg (SAT)] | Corrects magenta color saturation. [−63]…[63] Factory setting: [6]
[Mg-B (SAT)] | Corrects the color saturation between magenta and blue. [−63]…[63] Factory setting: [5]
[B (SAT)] | Corrects blue color saturation. [−63]…[63] Factory setting: [0]
[B-Cy (SAT)] | Corrects the color saturation between blue and cyan. [−63]…[63] Factory setting: [−3]
[Cy (SAT)] | Corrects cyan color saturation. [−63]…[63] Factory setting: [−5]
[Cy-G (SAT)] | Corrects the color saturation between cyan and green. [−63]…[63] Factory setting: [0]
[G (SAT)] | Corrects green color saturation. [−63]…[63] Factory setting: [6]
[G-Yl (SAT)] | Corrects the color saturation between green and yellow. [−63]…[63] Factory setting: [−2]
[Yl (SAT)] | Corrects yellow color saturation. [−63]…[63] Factory setting: [14]
[Yl-Yl-R (SAT)] | Corrects the color saturation between yellow and “colors between yellow and red”. [−63]…[63] Factory setting: [25]
[Yl-R (SAT)] | Corrects the color saturation between yellow and red. [−63]…[63] Factory setting: [28]
[Yl-R-R (SAT)] | Corrects the color saturation between “colors between yellow and red” and red. [−63]…[63] Factory setting: [43]
[R (PHASE)] | Corrects the red hue. [−63]…[63] Factory setting: [0]
[R-R-Mg (PHASE)] | Corrects the hue between red and “colors between red and magenta”. [−63]…[63] Factory setting: [10]
[R-Mg (PHASE)] | Corrects the hue between red and magenta. [−63]…[63] Factory setting: [5]
[Mg (PHASE)] | Corrects the magenta hue. [−63]…[63] Factory setting: [3]
[Mg-B (PHASE)] | Corrects the hue between magenta and blue. [−63]…[63] Factory setting: [4]
[B (PHASE)] | Corrects the blue hue. [−63]…[63] Factory setting: [0]
[B-Cy (PHASE)] | Corrects the hue between blue and cyan. [−63]…[63] Factory setting: [0]
[Cy (PHASE)] | Corrects the cyan hue. [−63]…[63] Factory setting: [12]
[Cy-G (PHASE)] | Corrects the hue between cyan and green. [−63]…[63] Factory setting: [15]
[G (PHASE)] | Corrects the green hue. [−63]…[63] Factory setting: [10]
[G-Yl (PHASE)] | Corrects the hue between green and yellow. [−63]…[63] Factory setting: [10]
[Yl (PHASE)] | Corrects the yellow hue. [−63]…[63] Factory setting: [6]
[Yl-Yl-R (PHASE)] | Corrects the hue between yellow and “colors between yellow and red”. [−63]…[63] Factory setting: [22]
[Yl-R (PHASE)] | Corrects the hue between yellow and red. [−63]…[63] Factory setting: [7]
[Yl-R-R (PHASE)] | Corrects the hue between “colors between yellow and red” and red. [−63]…[63] Factory setting: [13]

NOTE

- When saving or reading setup files from an SD memory card, you can save items with an [S] and items without an [S] separately. Items with an [S] in front of the item name are the targets for [PAINT([S]SELECT)] in the main menu → [FILE] → [SETUP DATA SELECT]. Items without an [S] are targets for [PAINT(LEVEL)].

## [LOW SETTING]

Item | Description of settings
--- | ---
[[S] MASTER GAIN] | Selects the master gain. [−6dB], [−3dB], [0dB], [3dB], [6dB], [9dB], [12dB], [15dB], [18dB], [21dB], [24dB], [27dB], [30dB] Factory setting: [0dB]
[H.DTL LEVEL] | Sets the horizontal detail correction level. [0]…[63] Factory setting: [12]
[V.DTL LEVEL] | Sets the vertical detail correction level. [0]…[31] Factory setting: [15]
[DTL CORING] | Sets the detail noise removal level. [0]…[60] Factory setting: [1]
[H.DTL FREQ.] | Selects the horizontal detail frequency. [0]…[31] Factory setting: [18]
[LEVEL DEPEND.] | Sets [LEVEL DEPEND.]. Compresses the details of dark areas when Y detail is emphasized. Details of bright areas are also compressed if the value is large. [0]…[5] Factory setting: [1]
[MASTER GAMMA] | Sets the master gamma in 0.01 steps. [0.30]…[0.75] Factory setting: [0.45]
[BLACK GAMMA] | Sets the gamma curves of dark areas. [−8]…[−1]: Compresses the dark areas. [OFF]: Standard state [1]…[8]: Expands the dark areas. Factory setting: [OFF]
[B. GAMMA RANGE] | Sets the maximum level of compression/expansion. [1]: About 20% [2]: About 30% [3]: About 40% Factory setting: [1]
[[S] MATRIX TABLE] | Selects the color collection table for the linear matrix. [A], [B], [OFF] Factory setting: [A]
[[S] COLOR CORRECT] | Switches the 15-axis independent color correction on/off. [ON], [OFF] Factory setting: [ON]

NOTE

- When saving or reading setup files from an SD memory card, you can save items with an [S] and items without an [S] separately. Items with an [S] in front of the item name are the targets for [PAINT([S]SELECT)] in the main menu → [FILE] → [SETUP DATA SELECT]. Items without an [S] are targets for [PAINT(LEVEL)].

- [−6dB] in [[S] MASTER GAIN] cannot be selected when [NORMAL] is set in main menu → [PAINT] → [[S] CAMERA SETTING] → [SHOOTING MODE].

- A coloration phenomenon may occur in videos of high-brightness areas if shooting was done with the master gain set to [−6dB] or [−3dB]. After switching the <OUTPUT>/<AUTO KNEE> selection switch to <CAM>/<OFF> and setting [ON] in the main menu → [PAINT] → [KNEE/LEVEL] → [[S] MANUAL KNEE], you can reduce the coloration phenomenon by changing the following menu items:

  - Reduce the [KNEE MASTER SLOPE] value of [KNEE/LEVEL] when [HD], [SD], [FILMLIKE1], [FILMLIKE2], or [FILMLIKE3] is selected in the main menu → [PAINT] → [GAMMA] → [GAMMA MODE SEL].

  - Reduce the [F-REC DYNAMIC LVL] value of [GAMMA] when [FILM-REC] is selected in main menu → [PAINT] → [GAMMA] → [GAMMA MODE SEL].

  - Reduce the [V-REC KNEE SLOPE] value of [GAMMA] when [VIDEO-REC] is selected in the main menu → [PAINT] → [GAMMA] → [GAMMA MODE SEL].

## [MID SETTING]

Item | Description of settings
--- | ---
[[S] MASTER GAIN] | Selects the master gain. [−6dB], [−3dB], [0dB], [3dB], [6dB], [9dB], [12dB], [15dB], [18dB], [21dB], [24dB], [27dB], [30dB] Factory setting: [6dB]
[H.DTL LEVEL] | Sets the horizontal detail correction level. [0]…[63] Factory setting: [8]
[V.DTL LEVEL] | Sets the vertical detail correction level. [0]…[31] Factory setting: [12]
[DTL CORING] | Sets the detail noise removal level. [0]…[60] Factory setting: [8]
[H.DTL FREQ.] | Selects the horizontal detail frequency. [0]…[31] Factory setting: [18]
[LEVEL DEPEND.] | Sets [LEVEL DEPEND.]. Compresses the details of dark areas when Y detail is emphasized. Details of bright areas are also compressed if the value is large. [0]…[5] Factory setting: [1]
[MASTER GAMMA] | Sets the master gamma in 0.01 steps. [0.30]…[0.75] Factory setting: [0.45]
[BLACK GAMMA] | Sets the gamma curves of dark areas. [−8]…[−1]: Compresses the dark areas. [OFF]: Standard state [1]…[8]: Expands the dark areas. Factory setting: [OFF]
[B. GAMMA RANGE] | Sets the maximum level of compression/expansion. [1]: About 20% [2]: About 30% [3]: About 40% Factory setting: [1]
[[S] MATRIX TABLE] | Selects the color collection table for the linear matrix. [A], [B], [OFF] Factory setting: [A]
[[S] COLOR CORRECT] | Switches the 15-axis independent color correction on/off. [ON], [OFF] Factory setting: [ON]

NOTE

- When saving or reading setup files from an SD memory card, you can save items with an [S] and items without an [S] separately. Items with an [S] in front of the item name are the targets for [PAINT([S]SELECT)] in the main menu → [FILE] → [SETUP DATA SELECT]. Items without an [S] are targets for [PAINT(LEVEL)].

- [−6dB] in [[S] MASTER GAIN] cannot be selected when [NORMAL] is set in main menu → [PAINT] → [[S] CAMERA SETTING] → [SHOOTING MODE].

## [HIGH SETTING]

Item | Description of settings
--- | ---
[[S] MASTER GAIN] | Selects the master gain. [−6dB], [−3dB], [0dB], [3dB], [6dB], [9dB], [12dB], [15dB], [18dB], [21dB], [24dB], [27dB], [30dB] Factory setting: [12dB]
[H.DTL LEVEL] | Sets the horizontal detail correction level. [0]…[63] Factory setting: [6]
[V.DTL LEVEL] | Sets the vertical detail correction level. [0]…[31] Factory setting: [10]
[DTL CORING] | Sets the detail noise removal level. [0]…[60] Factory setting: [12]
[H.DTL FREQ.] | Selects the horizontal detail frequency. [0]…[31] Factory setting: [18]
[LEVEL DEPEND.] | Sets the [LEVEL DEPEND.]. Compresses the details of dark areas when Y detail is emphasized. Details of bright areas are also compressed if the value is large. [0]…[5] Factory setting: [1]
[MASTER GAMMA] | Sets the master gamma in 0.01 steps. [0.30]…[0.75] Factory setting: [0.55]
[BLACK GAMMA] | Sets the gamma curves of dark areas. [−8]…[−1]: Compresses the dark areas. [OFF]: Standard state [1]…[8]: Expands the dark areas. Factory setting: [OFF]
[B. GAMMA RANGE] | Sets the maximum level of compression/expansion. [1]: About 20% [2]: About 30% [3]: About 40% Factory setting: [1]
[[S] MATRIX TABLE] | Selects the color collection table for the linear matrix. [A], [B], [OFF] Factory setting: [A]
[[S] COLOR CORRECT] | Switches the 15-axis independent color correction on/off. [ON], [OFF] Factory setting: [ON]

NOTE

- When saving or reading setup files from an SD memory card, you can save items with an [S] and items without an [S] separately. Items with an [S] in front of the item name are the targets for [PAINT([S]SELECT)] in the main menu → [FILE] → [SETUP DATA SELECT]. Items without an [S] are targets for [PAINT(LEVEL)].

- [−6dB] in [[S] MASTER GAIN] cannot be selected when [NORMAL] is set in main menu → [PAINT] → [[S] CAMERA SETTING] → [SHOOTING MODE].

## [ADDITIONAL DTL]

Item | Description of settings
--- | ---
[KNEE APE LVL] | Changes the detail level of high-brightness areas. [OFF], [1]…[5] Factory setting: [2]
[DTL GAIN(+)] | Changes the level of + (upper) direction of detail. [−31]…[31] Factory setting: [0]
[DTL GAIN(−)] | Changes the level of − (lower) direction of detail. [−31]…[31] Factory setting: [0]
[DTL CLIP] | Sets the level at which detail signals will be clipped. [0]…[63] Factory setting: [0]
[DTL SOURCE] | Sets the ratio of RGB signal components that will create the detail. [(R+G)/2], [(G+B)/2], [(2G+R+B)/4], [(3G+R)/4], [R], [G] Factory setting: [(R+G)/2]
[MASTER DTL] | Changes the master detail level. [−31]…[31] Factory setting: [0]

## [SKIN TONE DTL]

Item | Description of settings
--- | ---
[[S] SKIN TONE DTL] | Selects the skin tone table that will display the skin tone detail. Create the skin tone table with [DETECT TABLE]. You can shoot smoother skin tones by displaying skin tone detail. Select one, two, or three skin tones from the [A], [B], and [C] tables. [A], [B], [C], [AB], [AC], [BC], [ABC], [OFF] Factory setting: [OFF] [SKIN TONE DTL] works independently from the details set in each item of [LOW SETTING], [MID SETTING], [HIGH SETTING], [ADDITIONAL DTL], and [[S] CAMERA SETTING].
[[S] ZEBRA VF] | Set to display a zebra pattern in the skin tone area displayed in the viewfinder screen. The zebra pattern is displayed when this item is set to [ON] and [SKIN TONE DTL] is open. The zebra pattern displays the area selected in [SKIN TONE DTL]. [ON], [OFF] Factory setting: [OFF]
[[S] ZEBRA SDI OUT1] | Set whether to display skin tone zebra in the SDI OUT1 signal. The zebra pattern is displayed when this item is set to [ON] and [SKIN TONE DTL] is open. The zebra pattern displays the area selected in [SKIN TONE DTL]. [ON], [OFF] Factory setting: [OFF]
[[S] ZEBRA MONI] | Set whether to display skin tone zebra in the monitor output (SDI OUT2, HDMI OUT, VIDEO OUT) signal. The zebra pattern is displayed when this item is set to [ON] and [SKIN TONE DTL] is open. The zebra pattern displays the area selected in [SKIN TONE DTL]. [ON], [OFF] Factory setting: [OFF]
[DETECT TABLE] | Selects the skin tone table of the subject that displays skin tone detail. [A], [B], [C] Factory setting: [A]
[SKIN TONE GET] | Obtains the color information of [A], [B], or [C] selected in [DETECT TABLE] from near the center marker. If executed, data from [I CENTER] to [Q PHASE] are automatically obtained. The obtained data becomes the table data of [A], [B], or [C] selected in [DETECT TABLE]. Multiple color information for [A], [B], and [C] cannot be obtained simultaneously.
[SKIN DTL EFFECT] | Sets the effective level of the skin tone detail. [0]…[63] Factory setting: [16]
[I CENTER] | Sets the center position of the upper I axis (setting the area that displays skin tone). [0]…[255] Factory setting: [35]
[I WIDTH] | Sets the width of the area that displays the skin tone of the upper I axis that focus on [I CENTER]. [0]…[255] Factory setting: [55]
[Q WIDTH] | Sets the width of the area that displays the skin tone of the upper Q axis that focus on [I CENTER]. [0]…[90] Factory setting: [10]
[Q PHASE] | Sets the phase of the area that displays the skin tone regarding to the Q-axis. [−180]…[179] Factory setting: [0]

- direction

+ direction

[Q WIDTH]

[I CENTER]

[I WIDTH]

[Q PHASE]

Skin tone area

NOTE

- When saving or reading setup files from an SD memory card, you can save items with an [S] and items without an [S] separately. Items with an [S] in front of the item name are the targets for [PAINT([S]SELECT)] in the main menu → [FILE] → [SETUP DATA SELECT]. Items without an [S] are targets for [PAINT(LEVEL)].

## [KNEE/LEVEL]

Item | Description of settings
--- | ---
[MASTER PED] | Sets the master pedestal. [−200]…[200] Factory setting: [16]
[[S] MANUAL KNEE] | Sets the mode when the <OUTPUT>/<AUTO KNEE> switch is <OFF>. This enables the [KNEE MASTER POINT]/[KNEE MASTER SLOPE] setting value when the switch is [ON]. [ON], [OFF] Factory setting: [ON]
[KNEE MASTER POINT] | Sets the knee point position in 0.5% steps. [70.0%]…[107.0%] Factory setting: [93.0%] The setting becomes invalid when [FILM-REC] or [VIDEO-REC] is selected in the main menu → [PAINT] → [GAMMA] → [GAMMA MODE SEL].
[KNEE MASTER SLOPE] | Sets the knee inclination. [0]…[99] Factory setting: [85] The setting becomes invalid when [FILM-REC] or [VIDEO-REC] is selected in the main menu → [PAINT] → [GAMMA] → [GAMMA MODE SEL].
[[S] WHITE CLIP] | Turns the white clip function [ON]/[OFF]. This enables the [WHITE CLIP LVL] setting value when the function is [ON]. [ON], [OFF] Factory setting: [ON]
[WHITE CLIP LVL] | Sets the white clip level. [90%]…[109%] Factory setting: [109%]
[A.KNEE POINT] | Sets the auto knee point position in 1% steps. This is enabled when the <OUTPUT>/<AUTO KNEE> switch is <CAM>/<ON>. [80%]…[107%] Factory setting: [90%]
[A.KNEE LVL] | Sets the auto knee level. [100]…[109] Factory setting: [107]
[A.KNEE RESPONSE] | Sets the auto knee response speed. The smaller the setting value, the faster the response speed is. [1]…[8] Factory setting: [4]
[CHROMA LEVEL] | Sets the chroma level of PR and PB signals. When this is set to [OFF], the color components of the video signal are removed. [OFF], [−99%]…[40%] Factory setting: [0%]
[DRS MODE] | Sets the effectiveness of DRS color preservation. [MODE1]: Sets the hue of high-brightness areas to its natural state. [MODE2]: Makes the hue of high-brightness areas more vivid. Factory setting: [MODE1]
[DRS EFFECT DEPTH] | Sets the compression level for the high-brightness areas of DRS. The higher the value, the higher the compression level of high-brightness areas becomes. [1], [2], [3] Factory setting: [1]
[[S] HI-COLOR SW] | Turns the mode that expands the color dynamic range [ON]/[OFF]. [ON], [OFF] Factory setting: [ON]
[HI-COLOR LVL] | Selects the level of the mode that expands the color dynamic range. [1]…[32] Factory setting: [32]

NOTE

- When saving or reading setup files from an SD memory card, you can save items with an [S] and items without an [S] separately. Items with an [S] in front of the item name are the targets for [PAINT([S]SELECT)] in the main menu → [FILE] → [SETUP DATA SELECT]. Items without an [S] are targets for [PAINT(LEVEL)].

## [GAMMA]

Item | Description of settings
--- | ---
[MASTER GAMMA] | Configure master gamma settings in 0.01 steps. [0.30]…[0.75] Factory setting: [0.45]
[R GAMMA] | Sets the gamma of Rch. [−15]…[15] Factory setting: [0]
[B GAMMA] | Sets the gamma of Bch. [−15]…[15] Factory setting: [0]
[GAMMA MODE SEL] | Selects the gamma curve. [HD]: The video gamma feature for HD (High Definition). [SD]: Increases gain in darker areas more than HD gamma. [FILMLIKE1]: Feature that reproduces more highlight areas compared to HD gamma. [FILMLIKE2]: Feature that reproduces more highlight areas compared to [FILMLIKE1]. [FILMLIKE3]: Feature that reproduces more highlight areas compared to [FILMLIKE2]. [FILM-REC]: The cine gamma feature for film. [VIDEO-REC]: The cine gamma feature for video. [HLG]: The hybrid log gamma feature. Factory setting: [HD] When [FILMLIKE3] is used, it is recommended to configure the following settings at the main menu → [PAINT] → [KNEE/LEVEL]. [[S] MANUAL KNEE]: [ON] [KNEE MASTER POINT]: [85.0%] [KNEE MASTER SLOPE]: [50] If set to [FILM-REC], [VIDEO-REC], or [HLG], auto knee is disabled.
[F-REC DYNAMIC LVL] | When [FILM-REC] is selected in [GAMMA MODE SEL], dynamic range is set. If an item other than [FILM-REC] is selected, no settings are changed. [200%], [300%], [400%], [500%], [600%] Factory setting: [600%]
[F-REC BLACK STR LVL] | When [FILM-REC] is selected in [GAMMA MODE SEL], black stretch is set. If an item other than [FILM-REC] is selected, no settings are changed. [0%]…[30%] Factory setting: [0%]
[V-REC KNEE SLOPE] | When [VIDEO-REC] is selected in [GAMMA MODE SEL], knee slope is set. If an item other than [VIDEO-REC] is selected, no settings are changed. [150%], [200%], [250%], [300%], [350%], [400%], [450%], [500%] Factory setting: [500%]
[V-REC KNEE POINT] | When [VIDEO-REC] is selected in [GAMMA MODE SEL], knee point is set. If an item other than [VIDEO-REC] is selected, no settings are changed. [30%]…[107%] Factory setting: [30%]

Image level

Luminosity

[SD]

[HD]

[FILMLIKE1]

[FILMLIKE2]

[FILMLIKE3]

[VIDEO-REC]

[FILM-REC]

## [[S] CAMERA SETTING]

Item | Description of settings
--- | ---
[SHOOTING MODE] | Selects the shooting mode according to the shooting environment. [NORMAL]: Selects normal sensitivity. (Appropriate when shooting in normal brightness.) [HIGH SENS.]: Selects high-sensitivity. (Appropriate when shooting in a dark environment.) [H.SENS.] is displayed on the viewfinder screen. Factory setting: [NORMAL] If [NORMAL] is selected, [−6dB] cannot be assigned to <LOW>/<MID>/<HIGH> on the <GAIN> switch. If changed from [HIGH SENS.] to [NORMAL], the following setting values also change. When [−6dB] is set in the main menu → [PAINT] → [LOW SETTING] → [[S] MASTER GAIN], it is changed to [−3dB]. When [−6dB] is set in the main menu → [PAINT] → [MID SETTING] → [[S] MASTER GAIN], it is changed to [−3dB]. When [−6dB] is set in the main menu → [PAINT] → [HIGH SETTING] → [[S] MASTER GAIN], it is changed to [−3dB].
[DETAIL] | Switches the detail signal [ON]/[OFF]. [ON], [OFF] Factory setting: [ON]
[2D LPF] | Sets a 2D low-pass filter to reduce cross colors. [ON]: Reduces cross colors. [OFF]: Does not reduce cross colors. Factory setting: [OFF] This item is displayed when in SD mode (480/59.94i and 576/50i).
[GAMMA] | Enables/disables gamma correction. [ON], [OFF] Factory setting: [ON]
[TEST SAW] | Enables/disables the test signal. [ON], [OFF] Factory setting: [OFF]
[FLARE] | Enables/disables flare correction. [ON], [OFF] Factory setting: [ON]
[H-F COMPE.] | Enables/disables aperture correction. [ON], [OFF] Factory setting: [ON]

NOTE

- All [[S] CAMERA SETTING] items are targets of [PAINT([S]SELECT)] in the main menu → [FILE] → [SETUP DATA SELECT].

Top of the page