- Top
- Description of Parts
- Warning and status display section

# Warning and status display section

1. <DISPLAY SELECT> button

   Switches the display of the LCD monitor. Press the <DISPLAY SELECT> button to switch between the image or thumbnail display and the status display.

2. <BACKLIGHT> button

   Controls the brightness of the LCD monitor.

   Every press of the button adjusts the brightness.

   NOTE

   - This setting is linked to setting of the main menu → [I/F SETUP] → [LCD MONITOR] → [BACKLIGHT]. The operation of the <BACKLIGHT> button is disabled while [BACKLIGHT] of the menu is set.

3. <WARNING> lamp (Warnings description list)

   Starts flashing or is illuminated if something unusual occurs in the memory.

4. <USB> lamp

   Lights when the camera is in the USB mode.

5. Back tally switch

   Controls the action of the back and rear tally lamps.

   <ON> | Enables the back and rear tally lamps.
   <OFF> | Disables the back and rear tally lamps.

6. Back tally lamp

   When the back tally switch is set to <ON>, the lamp acts in the same way as the front tally lamp at the viewfinder.

7. Rear tally lamp

   When the back tally switch is set to <ON>, the lamp acts in the same way as the back tally lamp.

Top of the page