- Top
- Menu Operations
- Menu list
- [CAMERA]

# [CAMERA]

These are items for changing the settings based on the condition of subject when the camera is operated.

These menu items cannot be set when the thumbnail screen is displayed.

## [CAMERA ID]

Item | Description of settings
--- | ---
[ID1] | Setting 1 of the camera ID to record to the color bars. Up to 10 characters may be used.
[ID2] | Setting 2 of the camera ID to record to the color bars. Up to 10 characters may be used.
[ID3] | Setting 3 of the camera ID to record to the color bars. Up to 10 characters may be used.

NOTE

- To clear the setting, execute the main menu → [FILE] → [INITIALIZE] → [LOAD FACTORY DATA].

## [SHUTTER SPEED]

Item | Description of settings
--- | ---
[SYNCHRO SCAN] | [SYNCHRO SCAN] is assigned as the shutter speed selected by the <SHUTTER> switch. [ON], [OFF] Factory setting: [ON]
[POSITION1] | The speed set in the main menu → [CAMERA] → [SHUTTER SELECT] → [POSITION1 SEL] is assigned as the shutter speed selected by the <SHUTTER> switch. [ON], [OFF] Factory setting: [ON]
[POSITION2] | The speed set in the main menu → [CAMERA] → [SHUTTER SELECT] → [POSITION2 SEL] is assigned as the shutter speed selected by the <SHUTTER> switch. [ON], [OFF] Factory setting: [ON]
[POSITION3] | The speed set in the main menu → [CAMERA] → [SHUTTER SELECT] → [POSITION3 SEL] is assigned as the shutter speed selected by the <SHUTTER> switch. [ON], [OFF] Factory setting: [ON]
[POSITION4] | The speed set in the main menu → [CAMERA] → [SHUTTER SELECT] → [POSITION4 SEL] is assigned as the shutter speed selected by the <SHUTTER> switch. [ON], [OFF] Factory setting: [ON]
[POSITION5] | The speed set in the main menu → [CAMERA] → [SHUTTER SELECT] → [POSITION5 SEL] is assigned as the shutter speed selected by the <SHUTTER> switch. [ON], [OFF] Factory setting: [ON]
[POSITION6] | The speed set in the main menu → [CAMERA] → [SHUTTER SELECT] → [POSITION6 SEL] is assigned as the shutter speed selected by the <SHUTTER> switch. [ON], [OFF] Factory setting: [ON]

## [SHUTTER SELECT]

Item | Description of settings
--- | ---
[POSITION1 SEL] | Sets the shutter speed in the main menu → [CAMERA] → [SHUTTER SPEED] → [POSITION1]. 50 Hz: [1/60], [1/120], [1/250], [1/500], [1/1000], [1/2000], [HALF], [180.0deg], [172.8deg], [144.0deg], [120.0deg], [90.0deg], [45.0deg] Factory setting: [1/60] 59.94 Hz: [1/100], [1/120], [1/250], [1/500], [1/1000], [1/2000], [HALF], [180.0deg], [172.8deg], [144.0deg], [120.0deg], [90.0deg], [45.0deg] Factory setting: [1/100]
[POSITION2 SEL] | Sets the shutter speed in the main menu → [CAMERA] → [SHUTTER SPEED] → [POSITION2]. 50 Hz: [1/60], [1/120], [1/250], [1/500], [1/1000], [1/2000], [HALF], [180.0deg], [172.8deg], [144.0deg], [120.0deg], [90.0deg], [45.0deg] Factory setting: [1/120] 59.94 Hz: [1/100], [1/120], [1/250], [1/500], [1/1000], [1/2000], [HALF], [180.0deg], [172.8deg], [144.0deg], [120.0deg], [90.0deg], [45.0deg] Factory setting: [1/120]
[POSITION3 SEL] | Sets the shutter speed in the main menu → [CAMERA] → [SHUTTER SPEED] → [POSITION3]. 50 Hz: [1/60], [1/120], [1/250], [1/500], [1/1000], [1/2000], [HALF], [180.0deg], [172.8deg], [144.0deg], [120.0deg], [90.0deg], [45.0deg] Factory setting: [1/250] 59.94 Hz: [1/100], [1/120], [1/250], [1/500], [1/1000], [1/2000], [HALF], [180.0deg], [172.8deg], [144.0deg], [120.0deg], [90.0deg], [45.0deg] Factory setting: [1/250]
[POSITION4 SEL] | Sets the shutter speed in the main menu → [CAMERA] → [SHUTTER SPEED] → [POSITION4]. 50 Hz: [1/60], [1/120], [1/250], [1/500], [1/1000], [1/2000], [HALF], [180.0deg], [172.8deg], [144.0deg], [120.0deg], [90.0deg], [45.0deg] Factory setting: [1/500] 59.94 Hz: [1/100], [1/120], [1/250], [1/500], [1/1000], [1/2000], [HALF], [180.0deg], [172.8deg], [144.0deg], [120.0deg], [90.0deg], [45.0deg] Factory setting: [1/500]
[POSITION5 SEL] | Sets the shutter speed in the main menu → [CAMERA] → [SHUTTER SPEED] → [POSITION5]. 50 Hz: [1/60], [1/120], [1/250], [1/500], [1/1000], [1/2000], [HALF], [180.0deg], [172.8deg], [144.0deg], [120.0deg], [90.0deg], [45.0deg] Factory setting: [1/1000] 59.94 Hz: [1/100], [1/120], [1/250], [1/500], [1/1000], [1/2000], [HALF], [180.0deg], [172.8deg], [144.0deg], [120.0deg], [90.0deg], [45.0deg] Factory setting: [1/1000]
[POSITION6 SEL] | Sets the shutter speed in the main menu → [CAMERA] → [SHUTTER SPEED] → [POSITION6]. 50 Hz: [1/60], [1/120], [1/250], [1/500], [1/1000], [1/2000], [HALF], [180.0deg], [172.8deg], [144.0deg], [120.0deg], [90.0deg], [45.0deg] Factory setting: [1/2000] 59.94 Hz: [1/100], [1/120], [1/250], [1/500], [1/1000], [1/2000], [HALF], [180.0deg], [172.8deg], [144.0deg], [120.0deg], [90.0deg], [45.0deg] Factory setting: [1/2000]

NOTE

- During remote control when connected to the extension control unit (AG-EC4G), the shutter settings will be the setting values saved in each unit.

## [USER SW]

Item | Description of settings
--- | ---
[USER MAIN] | (Select a function) Assigns the <USER MAIN> button. For selectable functions and an explanation of functions, refer to “Assigning functions to <USER> buttons”. Factory setting: [SLOT SEL]
(Detection time) Selects a response to accept when the <USER MAIN> button is pressed. [NORMAL]: Accepts immediately when pressed. [1sec]: Accepts when pressed and held down for approx. one second. Factory setting: [NORMAL]
[USER1] | (Select a function) Assigns the <USER1> button. For selectable functions and an explanation of functions, refer to “Assigning functions to <USER> buttons”. Factory setting: [S.GAIN]
(Detection time) Selects a response to accept when the <USER1> button is pressed. [NORMAL]: Accepts immediately when pressed. [1sec]: Accepts when pressed and held down for approx. one second. Factory setting: [NORMAL]
[USER2] | (Select a function) Assigns the <USER2> button. For selectable functions and an explanation of functions, refer to “Assigning functions to <USER> buttons”. Factory setting: [DS.GAIN]
(Detection time) Selects a response to accept when the <USER2> button is pressed. [NORMAL]: Accepts immediately when pressed. [1sec]: Accepts when pressed and held down for approx. one second. Factory setting: [NORMAL]
[SHOT MARK (U3)] | (Select a function) Assigns the <SHOT MARKER> button. For selectable functions and an explanation of functions, refer to “Assigning functions to <USER> buttons”. Factory setting: [SHOT MARK]
(Detection time) Selects a response to accept when the <SHOT MARKER> button is pressed. [NORMAL]: Accepts immediately when pressed. [1sec]: Accepts when pressed and held down for approx. one second. Factory setting: [NORMAL]
[TEXT MEMO (U4)] | (Select a function) Assigns the <TEXT MEMO> button. For selectable functions and an explanation of functions, refer to “Assigning functions to <USER> buttons”. Factory setting: [TEXT MEMO]
(Detection time) Selects a response to accept when the <TEXT MEMO> button is pressed. [NORMAL]: Accepts immediately when pressed. [1sec]: Accepts when pressed and held down for approx. one second. Factory setting: [NORMAL]
[USER5] | (Select a function) Assigns the <USER5> button. For selectable functions and an explanation of functions, refer to “Assigning functions to <USER> buttons”. Factory setting: [INHIBIT]
(Detection time) Selects a response to accept when the <USER5> button is pressed. [NORMAL]: Accepts immediately when pressed. [1sec]: Accepts when pressed and held down for approx. one second. Factory setting: [NORMAL]

## [SW MODE]

Item | Description of settings
--- | ---
[RET SW] | Sets the function when the <RET> button on the lens is pressed. [INHIBIT]: The <RET> button function is disabled. [REC CHECK]: Recording check function is enabled. Records can be checked of the last several seconds recorded. [CAM RET]: Return video function is enabled. While the <RET> button is pressed, the signal supplied to the <SDI IN> terminal can be checked on the viewfinder and LCD monitor. [ASSIST]: Turns the focus assist display [ON]/[OFF]. [D.ZOOM]: Digital zoom function is enabled. Digital zoom can be switched [ON]/[OFF]. [EVF CLR]: Selects whether to display video in the viewfinder in color or in black and white. [TEXT MEMO]: Text memo function is enabled. A text memo can be recorded to the frame selected when the button is pressed. [SHOT MARK]: Shot mark function is enabled. Press to add a shot mark, and press again to remove it. Factory setting: [REC CHECK] The return video is not displayed correctly when an image signal that differs from the video system of this camera. When the main menu → [I/F SETUP] → [GENLOCK] → [GENLOCK] is set to [INT], return video images may sometimes be skewed slightly in the horizontal direction. When switching between camera images and return video images, the image on the viewfinder and LCD monitor may be disrupted for an instant. This is not a malfunction.
[S.BLK LVL] | Sets the super black level. [−30], [−20], [−10], [OFF] Factory setting: [−10]
[AUTO KNEE SW] | Enables/disables auto knee function and DRS function. [DRS]: When the <AUTO KNEE> switch is in the <ON> position, DRS function is enabled. [ON]: When the <AUTO KNEE> switch is in the <ON> position, auto knee function is enabled. [OFF]: Even if the <AUTO KNEE> switch is in the <ON> position, both auto knee function and DRS function are not enabled. Factory setting: [ON]
[SHD,ABB SW CTL] | Sets whether to automatically adjust black shading when the <AUTO W/B BAL> switch is pressed and held down on the <ABB> side for two seconds or more. [ON], [OFF] Factory setting: [OFF]
[COLOR BARS] | Selects the color bar to use. [SMPTE]: Uses the color bar in the SMPTE standard. [FULL BARS]: Uses full color bars. [SPLIT]: Uses SPLIT color bars for SNG (Satellite News Gathering). [ARIB]: Uses ARIB standard color bars. Factory setting: [SMPTE]
[FOCUS ASSIST] | Selects the operation when [ASSIST] (focus assist function) is assigned to the <USER> button or the <RET> button. [EXPAND]: Expands the display of the center portion of the video. [IN RED]: Outlines the contour of the video in red. Factory setting: [EXPAND]
[EXPAND MODE] | Selects the method to cancel expanded display when [EXPAND] is selected in [FOCUS ASSIST]. [10SEC]: Cancels in 10 seconds. [HOLD]: Cancels when the button to which [ASSIST] is assigned is pressed. [UNTIL REC]: Cancels when recording starts. Expanded display is not available during recording. Factory setting: [10SEC] Regardless of this setting, expanded display is canceled when the button to which [ASSIST] is assigned is pressed.
[WFM] | Selects the type of waveform to be displayed on the viewfinder screen or LCD monitor when the <USER> buttons (<USER MAIN>/<USER1>/<USER2>) to which the waveform monitor function is assigned is pressed. [WAVE]: Displays as a waveform. [VECTOR]: Displays as a vector. [WAVE/VECTOR]: Each time the button is pressed, the display changes in order from no display → waveform display → vector display → no display. Factory setting: [WAVE]
[WFM DISP] | Selects whether to display the waveform monitor on the viewfinder or on the LCD monitor. [VF]: Displays on the viewfinder. [LCD]: Displays on the LCD monitor. [VF/LCD]: Displays on the viewfinder and the LCD monitor. Factory setting: [VF/LCD]
[S.GAIN OFF] | Selects a method to release super gain mode. [L/M/H]: Released by changing the <GAIN> switch or <S.GAIN> switch (<USER> button). [S.GAIN]: Released by the <S.GAIN> switch (<USER> button) only. Factory setting: [L/M/H]
[DS.GAIN OFF] | Selects a method to release digital super gain mode (accumulated gain). [L/M/H]: Released by changing the <GAIN> switch or <DS.GAIN> switch (<USER> button). [DS.GAIN]: Released by the <DS.GAIN> switch (<USER> button) only. Factory setting: [DS.GAIN]
[D.ZOOM x2] | Selects whether to enable 2x when digital zoom is assigned to the <USER> button of the camera. [ON], [OFF] Factory setting: [ON]
[D.ZOOM x3] | Selects whether to enable 3x when digital zoom is assigned to the <USER> button of the camera. [ON], [OFF] Factory setting: [ON]
[D.ZOOM x4] | Selects whether to enable 4x when digital zoom is assigned to the <USER> button of the camera. [ON], [OFF] Factory setting: [ON]
[FBC(SHUTTER ON)] | Selects whether to permit the operation of the flash band compensation (FBC) function when the <SHUTTER> switch is set to <ON>. [ENABLE]: Permits the operation of the flash band compensation function with the <USER> button. [DISABLE]: Forbids the operation of the flash band compensation function with the <USER> button. Factory setting: [DISABLE]
[RC CHECK SW] | Selects camera operation when the <REC CHK> button of the extension control unit is pressed. [REC CHECK]: Recording check function is enabled. [PLAY]: Performs playback. Factory setting: [REC CHECK]

## [WHITE BALANCE MODE]

Item | Description of settings
--- | ---
[FILTER INH] | Selects whether white balance memory (Ach or Bch) data is held or not held for each CC filter. [ON]: Holds Ach and Bch memory data (2 memories), regardless of the CC filter. [OFF]: Holds Ach and Bch memory data (8 memories), for each CC filter. Factory setting: [ON]
[SHOCKLESS AWB] | When the position of the <WHITE BAL> switch is changed, set the time until when the white balance starts at the changed position. [FAST]: Approx. 1 second [NORMAL]: Approx. 2 seconds [SLOW1]: Approx. 3 seconds [SLOW2]: Approx. 10 seconds [SLOW3]: Approx. 20 seconds [OFF]: Moves instantly. Factory setting: [NORMAL]
[AWB AREA] | Switches the detection area that automatically adjusts white balance. [25%]: Detects 25% of the area near screen center. [50%]: Detects 50% of the area near screen center. [90%]: Detects 90% of the screen area. Factory setting: [25%]
[AWB B] | Sets the function assigned to the <WHITE BAL> switch <B>. [MEM]: Records setting values when white balance is automatically adjusted, and operates using those values each time the <WHITE BAL> switch is moved to <B>. [ATW]: Assigns the auto tracking white balance function. Factory setting: [MEM]
[ATW SPEED] | Switches the control speed of auto tracking white balance function. [NORMAL], [SLOW], [FAST] Factory setting: [NORMAL]
[TEMP PRE SEL SW] | Selects whether to set the preset color temperature to be variable or to switch between [3200K]/[5600K]. Right after the value is changed, the preset color temperature is set to [3200K] (when the filter <A> is set). [VAR]: Switchable from [< 2300K] to [> 15000K]. [3.2K/5.6K]: Can be switched to [3200K] or [5600K]. Factory setting: [VAR]
[COLOR TEMP PRE] | Sets color temperature when the <WHITE BAL> switch is in the <PRST> position. Sets the preset color temperatures selected in [TEMP PRE SEL SW]. When [VAR] is selected for [TEMP PRE SEL SW]: [< 2300K]…[> 15000K] Factory setting: [3200K] When [3.2K/5.6K] is selected for [TEMP PRE SEL SW]: [3200K], [5600K] Factory setting: [3200K] The range of color temperature that can be set differs depending on the position of the <CC FILTER> dial. When a high color temperature is set, sometimes the value does not change even if the color temperature is changed.
[AWB A TEMP] | Sets color temperature when the <WHITE BAL> switch is in the <A> position. If the white balance is automatically adjusted in the <A> position, the color temperature at that time is recorded to the <WHITE BAL> switch <A> position. [< 2300K]…[> 15000K] Factory setting: [3200K]
[AWB B TEMP] | Sets color temperature when the <WHITE BAL> switch is in the <B> position. If the white balance is automatically adjusted in the <B> position, the color temperature at that time is recorded to the <WHITE BAL> switch <B> position. [< 2300K]…[> 15000K] Factory setting: [3200K]

## [USER SW GAIN]

Item | Description of settings
--- | ---
[S.GAIN] | Selects the gain to enable to the <SUPER GAIN> switch (<USER> button). [30dB], [36dB], [42dB] Set to be valid/invalid per gain value. All gain values are valid in the factory settings.
[DS.GAIN] | Selects the accumulated gain to enable to the <DS.GAIN> switch (<USER> button). [6dB], [10dB], [12dB], [15dB], [20dB], [24dB], [28dB], [34dB] Set to be valid/invalid per gain value. The gain value of [20dB] or lower is valid in the factory setting. When [DS.GAIN] function is operating, the shutter mode is [OFF].

## [LENS/IRIS]

Item | Description of settings
--- | ---
[A.IRIS LEVEL] | Sets the auto iris target value. [0]…[100] Factory setting: [50]
[A.IRIS PEAK/AVE] | Sets the ratio included in the peak for auto iris standard. Larger ratios correspond to a peak within the IRIS detection window, and smaller ones correspond to average values within the IRIS detection window. [0]…[100] Factory setting: [30]
[A.IRIS WINDOW] | Selects the auto iris detection window. [NORM1]: Window that is near screen center. [NORM2]: Window that is near screen bottom. [CENTER]: Window that is a spot in the screen center. Factory setting: [NORM1]
[S.IRIS LEVEL] | Sets the super iris (backlight compensation) target value. [0]…[100] Factory setting: [70]
[IRIS GAIN] | Selects the IRIS GAIN adjustment side. [CAM], [LENS] Factory setting: [LENS] When using the lenses with extenders (such as x2 and x0.8) sold prior to the FUJINON DIGI POWER types, set to [LENS] with the extender inserted, and operate IRIS correction control. If set to [CAM], the IRIS control of the camera will no longer function correctly.
[IRIS GAIN VALUE] | Selects the [IRIS GAIN] adjustment value. When [CAM] is selected in [IRIS GAIN], this setting is enabled. [1]…[20] Factory setting: [10]

## [AGC]

Item | Description of settings
--- | ---
[AGC] | Selects [ON]/[OFF] for [AGC] function that automatically adjusts camera gain. [ON], [OFF] Factory setting: [OFF]
[AGC LIMIT] | Sets the maximum gain value during [AGC] operation. [3dB], [6dB], [12dB], [18dB] Factory setting: [12dB]
[AGC POINT] | Sets the F value to switch control to [AGC] from auto iris during [AGC] operation. [F5.6], [F4.0], [F2.8] Factory setting: [F2.8]

Top of the page