- Top
- Shooting
- Dual codec recording

# Dual codec recording

Recording in different formats for main recording and sub recording can be performed on the camera.

The HD proxy with resolution of 1920×1080 AVC-LongG 6 format, and multiple SD proxies with different resolution can be selected for sub recording. For the recording format that can record in dual codec, refer to “Multi formats”.

Video can be saved in high-resolution H.264/AVC format as well as MPEG4 format. For audio, besides AAC format, uncompressed audio (LPCM) is supported.

In addition to the traditional MPEG4 format, the MOV format more suitable for nonlinear editing is available.

Video files, audio files, and real-time metadata file (time code, user bits) can be recorded to the P2 card and SD memory card at the same time.

The recorded materials can be saved as a smaller data file to allow efficient clip check or editing.

Setting the dual codec
Recording the proxy data
Recording to the SD memory card
Checking the proxy data
Error displays about proxy data recordings
Top of the page