- Top
- Connecting to External Devices
- Connecting to the extension control unit (AG-EC4G)

# Connecting to the extension control unit (AG-EC4G)

- Connect the extension control unit AG-EC4G (optional) to remote-control some functions.

- When you connect AG-EC4G and set the <POWER> switch of the camera to < > (ON) and <POWER> switch of AG-EC4G to <ON>, the camera automatically transitions to the remote control mode.

- Remove AG-EC4G, or ensure the AG-EC4G <POWER> switch is <OFF> to release remote control mode.

AG-EC4G

<REMOTE> terminal

Switch functionality in remote control mode
Recording and playback operations in remote control mode
Remote control unit connected to the camera

NOTE

- The status adjusted with AG-EC4G connected will always be recorded on the camera. The setting of the <DATA SAVE> switch for AG-EC4G is currently disabled.

- When the dedicated cable is connected or disconnected, set the <POWER> switch of the camera to < > (standby) and the <POWER> switch of AG-EC4G always to <OFF>.

- Use a cable or optional cable that is dedicated for AG-EC4G. Otherwise, a malfunction may result.

- For details on the current from the <REMOTE> terminal, refer to “Details of the connector signals”.

- For details, refer to the Operating Instructions of AG-EC4G.

Top of the page