- Top
- Shooting
- Basic procedures
- Shooting and recording switch settings

# Shooting and recording switch settings

After turning on the power and inserting the P2 card, set the switches as follows before starting operations.

1. <USER MAIN> button

   Set to the card slot for recording target.

2. <GAIN> switch

   Normally, set this to <L> (0 dB). If it is too dark, set the gain to an appropriate value.

3. <OUTPUT>/<AUTO KNEE> switch

   Set this switch to <CAM>/<ON>.

4. <TCG> switch

   Set this switch to <F-RUN> or <R-RUN>.

5. <AUDIO SELECT CH1/3>, <AUDIO SELECT CH2/4> switches

   Set these switches to <AUTO>.

NOTE

- The [SLOT SEL] function is assigned to the <USER MAIN> button in the factory setting. You can switch to the P2 card to be recorded from two or more inserted P2 cards.

  When the P2 to record to is switched, the number of the card slot in which the P2 card to be recorded to is inserted is displayed on the P2 remaining card capacity indicator in the viewfinder. (For details on indications in the viewfinder, refer to “Configuration of status display on viewfinder screen”.)

- The [SLOT SEL] is enabled also during recording. The [SLOT SEL] indicator flashes in the viewfinder until switching of the P2 card to be recorded to is completed. If the card could not be switched immediately after recording is started or immediately after the P2 card is switched, [SLOT SEL INVALID] will be displayed.

- Switch the recording media between P2 memory cards (slots 1, 2) and microP2 memory cards (slots 3, 4) from the main menu → [REC/PB] → [REC/PB SETUP] → [REC MEDIA]. [REC MEDIA] can also be assigned to the <USER> button.

Top of the page