- Top
- Shooting
- Multi formats
- Selecting video output

# Selecting video output

The video output method can be selected.

Video output, etc. can be selected by the setting of [OUTPUT SEL] in the main menu → [I/F SETUP] and the setting of [DOWNCON SETTING] → [DOWNCON MODE].

Menu item | Description of settings
--- | ---
[SDI2/HDMI OUT] | Selects the system mode signal method or down converter output for output from the <SDI OUT2> and <HDMI OUT> terminals.
[1080P SDI2/HDMI OUT] | Selects whether to convert output signals from the monitor output terminals (<SDI OUT2>, <HDMI OUT>) to 1080i at 1080P.
[3G-SDI OUT] | Selects the 3G-HD SDI signal type output from the <SDI OUT1> and <SDI OUT2> terminals from [LEVEL-A] or [LEVEL-B] at 1080P.
[DOWNCON MODE] | Selects the screen type for down-conversion output (composite and SD SDI output) at 1080P, 1080i, or 720P.

## Selecting video output from each terminal

[LINE&FREQ] | Monitor output setting | Video output
--- | --- | ---
[SDI2/HDMI OUT] | [1080P SDI2/HDMI OUT] | <SDI OUT1> terminal | <SDI OUT2> terminal | <HDMI OUT> terminal | <VIDEO OUT> terminal
[1080-59.94P] | [SYSTEM MODE] | [1080P] | 1080/59.94P* | 1080/59.94P* | 1080/59.94P | 480/59.94i
[1080i] | 1080/59.94i | 1080/59.94i
[DOWNCON] | Disabled | 480/59.94i | 480/59.94P
[1080-50P] | [SYSTEM MODE] | [1080P] | 1080/50P* | 1080/50P* | 1080/50P | 576/50i
[1080i] | 1080/50i | 1080/50i
[DOWNCON] | Disabled | 576/50i | 576/50P
[1080-59.94i] | [SYSTEM MODE] | — | 1080/59.94i | 1080/59.94i | 1080/59.94i | 480/59.94i
[DOWNCON] | 480/59.94i | 480/59.94P
[1080-50i] | [SYSTEM MODE] | — | 1080/50i | 1080/50i | 1080/50i | 576/50i
[DOWNCON] | 576/50i | 576/50P
[1080-23.98PsF] | [SYSTEM MODE] | [1080P] | 1080/23.98PsF* | 1080/59.94P* | 1080/59.94P | 480/59.94i
[1080i] | 1080/59.94i | 1080/59.94i
[DOWNCON] | Disabled | 480/59.94i | 480/59.94i
[720-59.94P] | [SYSTEM MODE] | — | 720/59.94P | 720/59.94P | 720/59.94P | 480/59.94i
[DOWNCON] | 480/59.94i | 480/59.94i
[720-50P] | [SYSTEM MODE] | — | 720/50P | 720/50P | 720/50P | 576/50i
[DOWNCON] | 576/50i | 576/50P
[480-59.94i] | — | — | 480/59.94i | 480/59.94i | 480/59.94P | 480/59.94i
[576-50i] | — | — | 576/50i | 576/50i | 576/50P | 576/50i

Output type can be selected from [LEVEL-A] or [LEVEL-B] in the main menu → [I/F SETUP] → [OUTPUT SEL] → [3G-SDI OUT]. This item is set to [LEVEL-B] in the factory setting.

Top of the page