- Top
- Shooting
- Viewfinder status display
- Display modes and setting changes/adjustment result messages

# Display modes and setting changes/adjustment result messages

You can select how messages are displayed in the viewfinder and how messages for notifying the details of changes to settings and adjustment results are displayed. For example, whether to display or hide some items can be selected in the main menu → [VF] → [VF DISPLAY] → [DISP MODE]. For details on operation methods, refer to “Setting menu basic operations”.

#### Setting changes/adjustment result messages and [DISP MODE] settings

(✓: Display, —: hide)

Status for displaying messages | Message | [DISP MODE] setting
--- | --- | ---
[1] | [2] | [3]
When the <CC FILTER> dial/<ND FILTER> dial selection is changed | [FILTER:n] ([n] = [1], [2], [3], [4]), [m] ([m] = [A], [B], [C], [D]) | — | — | ✓
When the gain setting is changed | [GAIN:ndB] ([n] = [−6], [−3], [0], [3], [6], [9], [12], [15], [18], [21], [24], [27], [30]) | — | — | ✓
When the <WHITE BAL> switch setting is changed | [WHITE:n] ([n] = [A], [B], [PRE]) | — | — | ✓
When the <OUTPUT>/<AUTO KNEE> selector switch is set to <ON> or <OFF> | [AUTO KNEE:ON] (or [OFF]) | — | ✓ | ✓
When the shutter speed/mode setting is changed | [SS:1/100] (or [1/60], [1/120], [1/250], [1/500], [1/1000], [1/2000], [HALF], [.d], [1/.] or [.d]) | — | ✓ | ✓
When white balance is adjusted | Example) [AWB A OK 3.2 K] | — | ✓ | ✓
When black balance is adjusted | Example) [ABB OK] | — | ✓ | ✓
When the extender is selected | Example) [EXTENDER ON] | — | — | ✓
When the <USER> button is selected | Example) [UM:S.GAIN 30dB] | — | ✓ | ✓
When the marker select function is selected | Example) [MKR:A] | — | — | ✓
When in the iris override mode | Example) [++F5.6] | — | ✓ | ✓
When the CAC lens is mounted or unmounted | Example) [CAC LENS DATA INVALID] | — | ✓ | ✓

Top of the page