- Top
- Menu Operations
- Menu list
- [OPTION MENU]

# [OPTION MENU]

## [NETWORK MODE]

This menu brings together the items for the FTP client function, rec during upload function, and the streaming function in the main menu.

The settings are the same as each item in the main menu.

Item
[CODEC USAGE]
[FTP MODE] | [FTP CLIENT SERVICE] | [SETTING DATA]
|  | [SERVER URL]
|  | [LOGIN USER]
|  | [LOGIN PASSWORD]
|  | [SSH]
|  | [SSH PORT]
|  | [LOAD (SD CARD)]
|  | [SAVE (SD CARD)]
|  | [REC DURING UPLOAD]
|  | [AUTO UPLOAD]
|  | [UPLOAD LIST]
|  | [SAVE LOG (SD CARD)]
| [DUAL CODEC SETUP] | [PROXY REC MODE]
|  | [TC SUPER]
|  | [PROXY DISP]
[STREAMING MODE] | [STREAMING SETTING] | [START TRIGGER]
|  | [SETTING DATA]
|  | [SERVER ADDR.]
|  | [RTSP PORT]
|  | [LOAD (SD CARD)]
|  | [SAVE (SD CARD)]
|  | [START]
| [DUAL CODEC SETUP] | [STREAMING MODE]
|  | [QoS MAX RATE]
|  | [QoS MIN RATE]
|  | [STREAMING LATENCY]
[NETWORK SEL]
[LAN PROPERTY] | [MAC ADDRESS]
| [DHCP]
| [IP ADDRESS]
| [SUBNET MASK]
| [DEFAULT GATEWAY]
| [PRIMARY DNS]
| [SECONDARY DNS]
| [DHCP SERVER]
[WIRELESS PROPERTY] | [MAC ADDRESS]
| [TYPE]
| [SSID INPUT MODE]
| [SSID]
| [BAND]
| [CHANNEL (2.4GHz)]
| [CHANNEL (5GHz)]
| [ENCRYPTION]
| [ENCRYPT KEY]
| [DHCP]
| [IP ADDRESS]
| [SUBNET MASK]
| [DEFAULT GATEWAY]
| [PRIMARY DNS]
| [SECONDARY DNS]
| [DHCP SERVER]
[4G/LTE PROPERTY] | [APN]
| [USER ID]
| [PASSWORD]
| [DIAL NO.]
[NETWORK TOOLS] | [LOG DISPLAY]
| [STATUS DISPLAY]
| [INITIALIZE]
| [PING]

## [OPTION]

Item | Description of settings
--- | ---
[ENG SECURITY] | Selects whether to place restrictions on opening and closing the menu screen. [ON]: Disables opening of menu items other than [USER MENU]. To release, consult your dealer. [OFF]: Opening and closing are not restricted. Factory setting: [OFF]
[FAN MODE] | Sets the fan operation mode. [AUTO]: If the camera internal temperature rises, the fan will automatically rotate. [OFF]: The fan does not rotate at all times. The warning [FAN STOPPED] is displayed. Factory setting: [AUTO] Once the power is turned off, this item is always set to [AUTO] the next time power is turned on. If operation continues while the fan is stopped, the internal temperature of the camera rises and it may not be able to record or play back normally. Normally, use the camera in [AUTO].

## [AREA SETTING]

Item | Description of settings
--- | ---
[AREA SELECT] | Select the region in which to use the camera before the initial use. [NTSC]: Selects an NTSC region other than Japan. [NTSC (J)]: Selects Japan. [PAL]: Selects the PAL region. Factory setting: [NTSC] For details, refer to “Setting the region of use (setting frame frequency, etc.) ”.

Top of the page