- Top
- Playback
- Thumbnail operations
- Thumbnail screen

# Thumbnail screen

Press the <THUMBNAIL> button to display the thumbnail screen on the LCD monitor. Press the <THUMBNAIL> button again to return to the regular display. Also, when changing from the regular display to the thumbnail screen display, all clips will be displayed on the thumbnail screen.

Press the <MENU> button on the thumbnail screen to enable thumbnail menu operations.

1. Status message

   A message showing the process status is displayed. [UPDATING] and the icon are displayed while the screen is being refreshed.

2. Card slot, storage device, and network status display

   The statuses of the P2 card, storage device, and network connection are displayed as follows:

   (Yellow) | Displayed when there is at least one defective clip that may be restored in the inserted P2 card. For details, refer to “Restoring clips”.
   (Red) | Displayed when there is at least one defective clip that cannot be restored in the inserted P2 card. Clips with this indicator displayed cannot be repaired. Delete the clip. If the clips cannot be deleted, format the P2 card. For details, refer to “Deleting clips”.
   (White) | The card slot number in which the P2 card is inserted is displayed in white.
   (Yellow) | The card slot number of the P2 card in which the clip in the cursor position is saved is displayed in yellow. If the clips are recorded across multiple P2 cards, all slot numbers of those cards that contain the clips are displayed. NOTE The frame turns red if the inserted P2 card is in any of the following conditions: [RUNDOWN CARD] The maximum number of overwrites on the P2 card has been exceeded. [DIR ENTRY NG CARD] The directory structure on the P2 card is not supported. [AUTH NG CARD] Indicates that the card is a microP2 memory card which cannot authenticate a CPS password.
   (Gray) | Displayed in gray when a storage device is not connected.
   (White) | Displayed in white when a storage device can be used.
   (Yellow) | Displayed in yellow when the thumbnails of clips in the storage device are displayed.
   (Red) | Displayed in red when a storage device is connected but cannot be used.
   (Gray) | Displayed in gray when the wired LAN is not activated properly.
   (White) | Displayed in white when the wired LAN is not connected.
   (Yellow) | Displayed in yellow while the wired LAN is connected.
   (Red) | Displayed in red when there is a problem with the connection of wired LAN.
   (Gray) | Displayed in gray when the wireless LAN is not activated properly.
   (White) | Displayed in white when the wireless LAN is not connected.
   (Yellow) | Displayed in yellow while the wireless LAN is connected.
   (Red) | Displayed in red when there is a problem with the connection of wireless LAN.
   (Gray) | Displayed in gray when the 4G/LTE USB modem is not activated properly.
   (White) | Displayed in white when the 4G/LTE USB modem is not connected.
   (Yellow) | Displayed in yellow when the 4G/LTE USB modem is connected. Signal strength is represented by yellow vertical bars.
   (Red) | Displayed in red when there is a problem with the 4G/LTE USB modem.
   (Gray) | Displayed in gray when upload has not started, or upload is complete.
   (Yellow) | Displayed in yellow during upload.
   (Red) | Displayed from when upload error occurred until when the next transfer starts.

   NOTE

   - When remote control is possible in an IP connection, “R” is displayed on the network status indicator.

   - The status display of the defective clip is not displayed in the thumbnail screen of the storage device or the thumbnail screen of the FTP.

3. Display mode

   Displays the types of the thumbnails to be displayed on the screen and the types of other information screens. To switch between displays, refer to “Thumbnail screen display settings”.

   [ALL] | Displays all clips.
   [SAME FORMAT] | Displays clips in the same format as the system format.
   [SELECT] | Displays clips selected with the <SET> button.
   [MARKER] | Displays clips with shot marks.
   [TEXT MEMO] | Displays clips with text memo data.
   [SLOT n] | Displays clips in the specified P2 card. (n: indicates slot number 1 to 2.)
   [NG CLIPS] | Displays defective clips.
   [P2/REMAIN] | Displays media information (remaining capacity).
   [P2/USED] | Displays media information (used capacity).
   [META DATA] | Displays the set metadata.

4. Simple properties display

   This displays the various properties of the clip on which the pointer is positioned. You can select the items to display from the menu. For details, refer to “Properties”.

   NOTE

   - If the maximum number of characters is exceeded, it will only display the maximum number of characters that can be displayed.

5. Thumbnail

   Displays the thumbnail recorded in each clip. This thumbnail can be changed using the [EXCH. THUMBNAIL] function.

   For details, refer to “Thumbnail screen display settings”.

6. Clip information display

   Displays any one of the time code [TC] at the start of clip recording/user bits [UB] at the start of clip recording/shooting time [TIME]/shooting date [DATE]/shooting date and time [DATE TIME]/clip name [CLIP NAME]/user clip name [USER CLIP NAME]/card slot number [SLOT]/time cord of the thumbnail [THUMBNAIL TC] according to the setting.

7. Recording mode

   Displays the recording mode for the clip on which the cursor is positioned.

8. System format

   Displays the format for the clip on which the cursor is positioned.

9. Duration

   Displays the clip length (duration) at the cursor position and the current rough playback position against the clip length.

10. Number of selected clips and playback time display and bonding device information display

    Displays the number of clips selected in the thumbnail screen and playback time of the clip when [THUMBNAIL INFO.] is selected in the main menu → [CLIP] → [THUMBNAIL SETUP] → [INFORMATION SEL.]. For details, refer to “Setting the number of clips and playback time display”.

    Displays the signal strength and the remaining battery of the bonding device when [BONDING DEV. INFO.] is selected in the main menu → [CLIP] → [THUMBNAIL SETUP] → [INFORMATION SEL.]. For details, refer to “Setting the bonding device information display”.

11. Clip number

    The number assigned to the clip on the P2 card is displayed, normally in the order from the earliest recording date and time. The clip numbers of clips that cannot be played are shown in red, and the unplayable indicator is also displayed.

    For details, refer to “Thumbnail screen display settings”.

12. Shot mark indicator

    Displayed for the clip of a thumbnail with a shot mark attached.

    For details, refer to “Shot mark recording function”.

13. Indicator for clips with proxy

    Displayed for clips with proxy attached.

14. Text memo indicator

    Displayed for clips with text memo data attached.

15. Edit copied clip indicator

    Displayed for the edit copied clip.

16. Wide clip indicator

    Displayed for clips recorded with the 16:9 aspect ratio. However, it does not accompany clips in HD format.

17. Incomplete clip indicator

    This is displayed when clips are saved across multiple P2 cards and either of the P2 cards is not inserted in a card slot.

18. / Defective clip indicator, Unknown clip indicator

    This is displayed for defective clips, which may result from various causes such as turning off the power during recording.

    Clips with yellow defective clip indicators can sometimes be restored.

    For details, refer to “Restoring clips”.

    Clips with red defective clip indicators cannot be restored and must be deleted. If the clip cannot be deleted, format the P2 card.

    is displayed for clips which differ in format from the P2 standard.

19. Rec during upload status indicator

    Rec during upload status indicator shows the status of maximum 100 clips registered in the upload list as follows.

    (Gray) | Displayed until upload starts.
    (Yellow) | Displayed during upload.
    (Green) | Displayed when upload is completed normally and registered in the upload list.
    (Red) | Displayed when transfer error occurred during upload and registered in the upload list.

20. [P.only] indicator

    This is displayed for a clip with only proxy not including the video data and audio data of main recording in the FTP explorer screen.

21. Thumbnail scroll bar

    Indicates which part of the whole thumbnail is currently being viewed.

Top of the page