- Top
- Shooting
- Adjusting and setting the LCD monitor
- Using the LCD monitor

# Using the LCD monitor

Push the <OPEN> button towards the right to open the LCD monitor.

Set the LCD monitor screen to the easiest-to-view position.

Rotate up to 180° in the lens direction and 90° in the direction towards you.

Display the screen brightness in the main menu → [I/F SETUP] → [LCD MONITOR] → [BRIGHTNESS], the color density of the screen in [COLOR LEVEL], and screen contrast in [CONTRAST].

Set whether to display the character of status display or the setting menu in the LCD monitor and viewfinder in the main menu → [I/F SETUP] → [LCD MONITOR] → [VF/LCD CHAR].

NOTE

- When closing the LCD monitor, be sure to close it firmly.

- Take care not to apply excessive force on the LCD monitor when it is opened. Doing so may result in a malfunction.

- Condensation sometimes forms on the LCD panel of the LCD monitor in locations subject to extreme temperature differences. If this happens, wipe with a soft, dry cloth.

- If the camera recorder is very cold, the LCD monitor will be slightly darker than normal immediately after the power is turned on. The screen will return to its regular brightness when the temperature inside increases.

Top of the page