- Top
- Network Settings
- Web Screen
- Using EasyIP Setup Tool Plus to set the unit’s settings

Using EasyIP Setup Tool Plus to set the unit’s settings

The settings related to the unit’s network can be set using the supplied EasyIP Setup Tool Plus.

When multiple of this unit are to be set, they each need to be set individually.

If setting cannot be done using the EasyIP Setup Tool Plus, make the individual settings for this unit and the personal computer in [NETWORK SETUP] in the camera menu.

“[NETWORK SETUP]”

NOTE If, after the network settings have been set, another device on the same network has the same IP address, the network operations will not be performed properly. Set the IP address in such a way that it does not duplicate an existing IP address. Do not set network settings from a multiple number of EasyIP Setup Tool Plus programs at the same time for a single camera. When connected from more than one PC, the settings of this unit can only be changed from the PC that was connected first. EasyIP Setup Tool Plus cannot be used from a different subnet via a router. Changes to the settings of this unit using the EasyIP Setup Tool Plus are performed with authentication from an account in the web screen, therefore changes are not possible if the initial account for the web screen is not yet set. “Displaying the web screen using a personal computer”

Setting Procedure

1. Start the EasyIP Setup Tool Plus.
2. Click the [Search] button.

- You can set the Network to be used for the search in the selection menu at the top of the screen.

3. Select the camera to configure and click the [Network Settings] button.

- The web screen for the selected camera is displayed when you click the [Web GUI] button.

4. Input the network items, and click the [Setup] button.

- Settings for DHCP, DNS, and Port No. are unsupported, so do not make settings for these.

5. Enter the user name and password registered in the web screen, then click the [OK] button.

- Enter the user name and password that was set for the initial account or was set in the User management screen [User mng.] in the web screen.

“Displaying the web screen using a personal computer”

“User management screen [User mng.]”

- After the [OK] button is clicked, it takes about 2 minutes for the settings in the unit to be completed. If this unit is turned off or the LAN cable is disconnected before the settings are completed, the settings will be invalidated. In this case, repeat the steps to set the settings.

NOTE The unit does not support IPv6. This unit does not support “Administrator Registration”, and “Firmware Update” from EasyIP Setup Tool Plus. When a firewall (including software) has been introduced, enable access to all the UDP ports. For details about EasyIP Setup Tool Plus, refer to the Help page.

Top of the page