- Top
- Menu Operations
- Menu list
- [MIC SETTING]

[MIC SETTING]

Item | Description of settings
[MIC1 (FRONT MIC) GAIN] | Sets the gain when there is a microphone input to the <MIC> terminal (front). [60dB], [40dB], [20dB] Factory setting: [60dB]
[MIC1 (FRONT MIC) AMP] | Sets the level of the input to the <MIC> terminal (front). [−20dB]…[+20dB] Factory setting: [0dB]
[MIC2 GAIN] | Sets the gain when there is a microphone input to the <MIC 2> terminal. [60dB], [40dB], [20dB] Factory setting: [60dB]
[MIC2 AMP] | Sets the level of the input to the <MIC 2> terminal. [−20dB]…[+20dB] Factory setting: [0dB]

Top of the page