- Top
- Menu Operations
- Menu list
- [INTERCOM SETTING]

[INTERCOM SETTING]

[INTERCOM]

Item | Description of settings
[INCOM TALK SETTING] | [MIC TYPE] | Selects the type of the intercom microphone. [DYN]: Dynamic type [ECM]: Condenser type [CBN]: Carbon type Factory setting: [DYN]
[MIC POWER] | Sets the on/off for the power supply to the intercom microphone. [OFF], [ON] Factory setting: [OFF]
[MIC GAIN] | Sets the volume of the intercom microphone. [−12dB]…[12dB] Factory setting: [0dB]
[SIDE TONE] | Sets the volume of the intercom microphone side tone. [OFF], [−36dB]…[0dB] (3 dB step) Factory setting: [−6dB]
[LEVEL VR] | Switches intercom level VR. [REAR], [FRONT] Factory setting: [REAR]
[PGM MIX] | Sets the on/off for the intercom PGM mix. [OFF], [ON] Factory setting: [ON]

Top of the page