- Top
- Preparation
- Attaching the viewfinder
- Attaching the rear viewfinder

Attaching the rear viewfinder

LCD viewfinder AK-HVF100G (optional) can be used with this camera.

For details on handling the LCD viewfinder, refer to the Operating Instructions of the viewfinder.

1. Turn off the power of the camera and the LCD viewfinder.
2. Press the lock release button and remove the connector cover. (Fig. 1)
3. Align the V-shaped protrusion of the LCD viewfinder with the V-shaped groove on the camera and slide it in until the lock is engaged. (Fig. 2)

NOTE When attaching the viewfinder, refrain from holding the hood of the LCD viewfinder.

Removing the rear viewfinder

1. Turn off the power of the camera and the LCD viewfinder.
2. While pressing the lock release button, slide off the LCD viewfinder.

NOTE When removing the viewfinder, refrain from holding the hood of the LCD viewfinder.

Top of the page