- Top
- Specifications
- Details of the connector signals

Details of the connector signals

OPT FIBER
| 1 | OPT-RX(Mark Band=IN)
2 | OPT-TX(Mark Band=OUT)
3 | DC190 V(C)
4 | DC190 V(H)
5 | STBY-SIG
6 | STBY-CONT
TAJIMI ELECTRONICS
| 1 | OPT-RX(Mark Band=IN)
2 | OPT-TX(Mark Band=OUT)
3 | STBY-SIG
4 | STBY-CONT
5 | DC190 V(H)
6 | DC190 V(C)
LEMO

INTERCOM
| 1 | TALK GND
2 | TALK
3 | RECEIVE GND
4 | RECEIVE CH1
5 | RECEIVE CH2
HA16PRH-5S (Hirose Electric Co.)

DC IN
| 1 | UNREG GND
2 | Not used
3 | Not used
4 | +12 V
HA16RA-4P(77) (Hirose Electric Co.)

MIC (front)
| 1 | GND
2 | AUDIO IN (H)
3 | AUDIO IN (C)
HA16PRM-3SG (Hirose Electric Co.)

MIC (rear)
| 1 | GND
2 | AUDIO IN (H)
3 | AUDIO IN (C)
HA16PRM-3SG (Hirose Electric Co.)

LENS
| 1 | RET-SW
2 | REC
3 | GND
4 | IRIS-AUTO
5 | IRIS-CONT
6 | UNREG +12 V+12 V
7 | IRIS-POSI
8 | IRIS-G-MAX
9 | EXT-POSI
10 | ZOOM-POSI
11 | FOCUS POSI/LENS RXD
12 | IRIS AUTO/LENS TXD
HR10A-10R-12SC (Hirose Electric Co.)

VF (front)
| 1 | UNREG -12 V
2 | UNREG -12 V
3 | +9 V
4 | VF-PB-OUT-GND
5 | VF-PR-OUT-GND
6 | VF-Y-OUT
7 | VF-Y-OUT-GND
8 | VF-CLK
9 | VF-WR
10 | VF-DATA
11 | UNREG-GND
12 | ZEBRA-SW
13 | PEAKING
14 | TA BOX ACT
15 | VF-PB-OUT
16 | VF-PR-OUT
17 | VF-SW3
18 | FRONT-VR
19 | TA TALLY
20 | GND
HR12-14RF-20SDL (Hirose Electric Co.)

VF (rear)
| 1 | VF-Y-OUT
2 | VF-PB-OUT
3 | VF-PR-OUT
4 | CAM DETECT
5 | I2C DATA
6 | R TALLY
7 | T TALLY
8 | UNREG +12 V
9 | UNREG +12 V
10 | UNREG +12 V
11 | VF-Y-OUT-GND
12 | VF-PB-OUT-GND
13 | VF-PR-OUT-GND
14 | AGND
15 | DGND
16 | Not used
17 | UNREG GND
18 | Not used
19 | FGND
20 | LCD ACT (Not used)
21 | Not used
22 | Not used
23 | PEAKING CONT (Not used)
24 | I2C CLK
25 | G TALLY
26 | VF P REQ
27 | RESERVED
28 | RESERVED
29 | RESERVED
D02F-29SF-N-F0 (Japan Aviation Electronics Industry)

Top of the page