- Top
- Preparation
- Connecting a microphone
- When mounting a microphone on the viewfinder (optional) for use

When mounting a microphone on the viewfinder (optional) for use

A microphone such as microphone kit AJ-MC700P (optional) can be mounted on the viewfinder.

1. Open the microphone holder. (Fig. 1)
2. Mount the microphone and tighten the clamp screw. (Fig. 2)
3. Insert the microphone cable into the cable clamp and connect it to the <MIC> terminal (front). (Fig. 3)
4. Set the <LINE/MIC/+48V> selector switch (<FRONT MIC>) to <MIC> or <+48V>.

Top of the page