- Top
- Maintenance
- Warning displays
- Camera warning displays

Camera warning displays

- When AWB (automatic white balance) is executed

[AWB BREAK] | Automatic white balance has been interrupted.
[AWB HIGH LIGHT NG] | Automatic white balance cannot be executed because the light amount is excessive. Set the light amount to an appropriate level.
[AWB LOW LIGHT NG] | Automatic white balance cannot be executed because the light amount is insufficient. Set the light amount to an appropriate level.
[AWB NG CHECK FILTER] | Automatic white balance cannot be executed because of erroneous filter position. Set the correct filter position.
[AWB RCH OUT RANGE] | The white balance convergence for red cannot be achieved. Shoot a uniformly white object on the screen, and execute AWB.
[AWB BCH OUT RANGE] | The white balance convergence for blue cannot be achieved. Shoot a uniformly white object on the screen, and execute AWB.

- When ABB (automatic black balance) is executed

[ABB BREAK] | Automatic black balance has been interrupted.
[ABB RCH OUT RANGE] | The black balance convergence for red cannot be achieved. Check if there are any errors in the image.
[ABB BCH OUT RANGE] | The black balance convergence for blue cannot be achieved. Check if there are any errors in the image.
[ABB GCH OUT RANGE] | The black balance convergence for green cannot be achieved. Check if there are any errors in the image.
[ABB NG] | The lens iris may not be closed.

- Executing black shading

[BSHD] | Black shading is executing.
[BSHD BRAK] | Black shading has been interrupted.
[BSHD NG] | An error has occurred with the black shading. Check if the lens is correctly closed.

Top of the page