- Top
- Menu Operations
- Menu configuration
- [MAIN MENU]

[MAIN MENU]

[DISPLAY SETUP] | Configures the settings for the details to be displayed in the viewfinder.
[SWITCH MODE] | Configures the function assigned to the switch.
[RETURN SETTING] | Configures the return switch and return signal name.
[INTERCOM SETTING] | Configures the details such as gain, etc. of each intercom.
[MIC SETTING] | Configures the audio settings.
[PAINT] | Configures the image settings.
[HDR-PAINT] | Configures the image settings during HDR.
[SYSTEM MODE] | Configures the system frequency and shooting mode.
[IN/OUT SELECT] | Configures the operation mode of the external input/output and each connection.
[NETWORK SETUP] | Configures the settings for the network.
[FILE] | Performs operations regarding handling of scene files and SD memory card.
[MAINTENANCE] | Adjusts the CAC and lens files.
[DIAGNOSTIC] | Displays the firmware version and energized time of the unit.

Top of the page