- Top
- Menu Operations
- Menu list
- [IN/OUT SELECT]

[IN/OUT SELECT]

Item | Description of settings
[CALL TALLY] | Sets whether the rear tally lamp is to be lit up when called. [OFF]: Turned off. [R]: Red tally lights up. [T]: Up tally lights up. [R&T]: Red tally and up tally light up. Factory setting: [OFF]
[TALLY GUARD] | Enables/disables automatic white balance, automatic black balance, and automatic setup when the tally lamp is lit. [OFF], [ON] Factory setting: [OFF]
[HD-SDI1 OUT] | Configures the video output from the <HD SDI1> terminal. [CAM]: Outputs camera images. [HD PROMPT]: Outputs HD prompter video images. Factory setting: [CAM]
[HD-SDI1 OUTPUT FORMAT] | Sets the signal format of the video output from the <HD SDI1> terminal. [1080i], [1080P], [720P] Factory setting: [1080i]
[HD-SDI1 OUTPUT ITEM] | Selects details of the characters superimposed on images output from the <HD SDI1> terminal. [MENU ONLY]: Displays only on the menu. [STATUS]: Displays all characters that are the same as in the viewfinder display. Factory setting: [MENU ONLY]
[HD-SDI1 CHAR] | Sets whether to superimpose characters on images output from the <HD SDI1> terminal. This cannot be set when the output format is [720P]. [OFF], [ON] Factory setting: [OFF]
[HD-SDI1 CHAR SIZE] | Sets the size of the characters superimposed on images output from the <HD SDI1> terminal. [LARGE], [SMALL] Factory setting: [SMALL]
[HD-SDI1 3G-SDI] | Sets the output format when [HD-SDI1 OUT] is [CAM] and when the image output from the <HD SDI1> terminal is 3G output. [LEVEL-A], [LEVEL-B] Factory setting: [LEVEL-B]
NOTE This is fixed to [LEVEL-A] when [HD-SDI1 OUT] is [HD PROMT].
[HD-SDI2 OUT] | Configures the video output from the <HD SDI2> terminal. [CAM]: Outputs camera images. [VF]: Outputs viewfinder images. [RET]: Outputs return images. [RET1], [RET2]: Outputs fixed return images. Factory setting: [VF]
[HD-SDI2 OUTPUT FORMAT] | Sets the signal format of the video output from the <HD SDI2> terminal. [1080i], [1080P], [720P] Factory setting: [1080i]
[HD-SDI2 OUTPUT ITEM] | Selects details of the characters superimposed on images output from the <HD SDI2> terminal. [MENU ONLY]: Displays only on the menu. [STATUS]: Displays all characters that are the same as in the viewfinder display. Factory setting: [MENU ONLY]
[HD-SDI2 CHAR] | Sets whether to superimpose characters on images output from the <HD SDI2> terminal. This cannot be set when the output format is [720P]. [OFF], [ON] Factory setting: [OFF]
[HD-SDI2 CHAR SIZE] | Sets the size of the characters superimposed on images output from the <HD SDI2> terminal. [LARGE], [SMALL] Factory setting: [SMALL]
[HD-SDI2 3G-SDI] | Sets the output format when [HD-SDI2 OUT] is [CAM] and when the image output from the <HD SDI2> terminal is 3G output. [LEVEL-A], [LEVEL-B] Factory setting: [LEVEL-B]
NOTE This is fixed to [LEVEL-A] when [HD-SDI2 OUT] is other than [CAM].
[AUX I/O] | Configures the video output from the <AUX> terminal. [PMT2 OUT], [HD TRUNK] Factory setting: [PMT2 OUT]
[T-BAR CONNECT] | Sets whether to connect the T-BAR unit. [OFF], [ON] Factory setting: [OFF]
[LENS I/F] | Sets the lens interface. [ANALOG], [SERIAL] Factory setting: [SERIAL]
[DISPLAY STATUS/BAR OSD] | [CAM ID CHARACTER] | Sets the camera name.

Top of the page