- Top
- Specifications
- Specifications
- Specifications

Specifications

General

Power DC12 V (when using an external power supply) DC190 V (when AK‑HCU250P/AK‑HCU250PS/AK‑HCU250E/AK‑HCU250ES is connected) Power consumption 82 W (maximum, when connecting to an external 12 V and including supply to an externally connected devices) 92 W (maximum, when AK-HCU250P/AK-HCU250PS/AK-HCU250E/AK-HCU250ES is conncected and including supply to an externally connected devices)

indicates safety information.

Ambient operating temperature | −10 °C to 45 °C (14 °F to 113 °F) (Preheating required under a temperature 0 °C (32 °F) or below)
Storage temperature | −20 °C to 60 °C (−4 °F to 140 °F)
Ambient operating humidity | 85% or less (relative humidity)
Weight | Approx. 4.0 kg (8.80 lbs.) (body only, excluding the accessories)
Dimensions (W×H×D) | Body only 151 mm × 267 mm × 369 mm (5-31/32 inches × 10-17/32 inches × 14-17/32 inches) (excluding protrusions)

Camera unit

Pickup device | 11.14 million pixels, CMOS Sensor
Optical filter | ND: Clear, 1/4, 1/16, 1/64
Lens mount | 2/3-type bayonet
Sensitivity | Two shooting modes [HIGH SENS]: F10 (59.94 Hz)/F11 (50 Hz) [NORMAL]: F6 (59.94 Hz)/F7 (50 Hz) 2000 lx, 3200 K, when white reflectivity is 89.9%
Horizontal modulation | 50% or above (27.5 MHz)
S/N | 62 dB or above
Horizontal resolution | HD: 1000 TV lines or above (center)
Gain switching | [NORMAL]: −6, −3, 0, 3, 6, 9, 12, 15, 18, 21, 24, 27, 30, 33, 36 [HIGH SENS]: −6, −3, 0, 3, 6, 9, 12, 15, 18, 21, 24, 27, 30, 33, 36
Shutter speed | [59.94i]/[59.94p] mode: 1/100, 1/120, 1/125, 1/250, 1/500, 1/1000, 1/1500, 1/2000 [29.97p] mode: 1/48, 1/50, 1/60, 1/96, 1/100, 1/120, 1/125, 1/250, 1/500, 1/1000, 1/1500, 1/2000 [23.98p] mode: 1/48, 1/50, 1/60, 1/96, 1/100, 1/120, 1/125, 1/250, 1/500, 1/1000, 1/1500, 1/2000 [50i]/[50p] mode: 1/60, 1/100, 1/125, 1/250, 1/500, 1/1000, 1/1500, 1/2000 [25p] mode: 1/48, 1/50, 1/60, 1/96, 1/100, 1/125, 1/250, 1/500, 1/1000, 1/1500, 1/2000
System format | 1920×1080/59.94p/50p/29.97p/25p/23.98p

Video input/output

<HD SDI1> terminal | BNC × 1 3G/1.5G-SDI: 0.8 V [p‑p], 75 Ω
<HD SDI2> terminal | BNC × 1 3G/1.5G-SDI: 0.8 V [p‑p], 75 Ω
<AUX> terminal | BNC × 1 Functions as <HD TRUNK> terminal/<PROMPTER> terminal by switching the setting in the menu <HD TRUNK>: 3G/1.5G-SDI: 0.8 V [p‑p], 75 Ω <PROMPTER>: VBS signal 1 V [p‑p], 75 Ω

Audio input/output

<MIC 2> terminal | XLR × 1, 3-pin, female type <LINE>/<MIC>/<+48V> switchable <LINE>: 0 dBu <MIC>: −60 dBu, −40 dBu, or −20 dBu menu can be selected
<MIC> terminal (front) | XLR × 1, 3-pin, female type <LINE>/<MIC>/<+48V> switchable <LINE>: 0 dBu <MIC>: −60 dBu, −40 dBu, or −20 dBu menu can be selected

Intercom

<INTERCOM> terminal | XLR × 1, 5-pin, female type

Other input/output

<OPT FIBER> terminal | Optical composite connector × 1
<LENS> terminal | 12-pin × 1
<VF> terminal | 20-pin × 1
<VF> terminal (rear) | 29-pin × 1
<DC IN> terminal | XLR × 1, 4-pin, DC 12 V
<LAN> terminal | RJ-45 × 1

The symbols on this product (including the accessories) represent the following:

AC DC

Top of the page