- Top
- Description of Parts
- Front side

Front side

1. Lens cable/microphone cable clamp
2. Used for securing the lens and microphone cables.
3. Lens mount (Bayonet type)
4. This is where the lens is mounted.
5. <SHUTTER> switch
6. This is the electronic shutter switch.
7. <OFF>: Disables the electronic shutter.
8. <ON>: Enables the electronic shutter.
9. <SEL>: Switches the shutter speed within the preset range.
10. This switch cannot be used when the CCU or ROP is connected to the camera.
11. <MIC> terminal (front)
12. Used to connect the microphone (optional).
13. When using, set the switch on the rear side as follows.
    - <LINE/MIC/+48V> selector switch (<FRONT MIC>): <MIC> or <+48V> (when using a phantom microphone)
14. <USER 1> button
15. A user-selected function can be assigned to this button. Pressing the button performs the assigned function.
16. Tripod mount
17. Used to attach the tripod adaptor SHAN-TM700 (optional) when mounting the camera on a tripod.
18. <INCOM LEVEL> dial (front)
19. Adjusts the volume of the intercom receiver.
20. Set [MAIN MENU] → [INTERCOM SETTING] → [INTERCOM] → [LEVEL VR] → [FRONT].
21. Lens lever
22. After the lens is mounted on the lens mount, this lever can be tightened to secure the lens.
23. <AUTO W/B BAL> switch
24. <AWB>: Automatically adjusts the white balance. When the white balance is automatically adjusted with the <WHITE BAL> switch on the side of the camera set to the <A> or <B> position, the white balance is adjusted in several seconds and the adjusted value is stored in the memory
25. <ABB>: Automatically adjusts the black balance. The operation performed when the CCU or ROP is connected to the camera can be set from [MAIN MENU] → [SWITCH MODE] → [W/B BAL SETTING].
26. <SELECT> dial button
27. Turning the <SELECT> dial button while the menu screen is displayed moves the cursor to a setting item. The menu setting can be confirmed by pressing the <SELECT> dial button. For details on operations, refer to “Menu operations”.

Top of the page