- Top
- Description of Parts
- Upper side

Upper side

1. Viewfinder front/back positioning lever
2. To adjust the front/back position of the viewfinder, loosen this lever and slide the viewfinder forwards or backwards to adjust the viewfinder to a position that enables easy viewing. After adjusting the viewfinder, turn the lever towards <LOCK> to lock the position.
3. Viewfinder left-right positioning ring
4. To adjust the left/right position of the viewfinder, loosen this lever and slide the viewfinder to the left or right to adjust the viewfinder to a position that enables easy viewing. Tighten the lever to clamp the viewfinder in place after adjusting.
5. Light shoe
6. Used to mount a video light, etc.
7. Microphone holder holes
8. Used to mount a microphone holder.
9. <PTT> switch
10. Used to switch the intercom microphone on/off. The function can be changed in [MAIN MENU] → [SWITCH MODE] → [USER SWITCH] → [GRIP PTT].
11. <RET> switch
12. Used to switch to the return A signal. The function can be changed in [MAIN MENU] → [SWITCH MODE] → [USER SWITCH] → [GRIP RET].
13. Accessory mounting hole
14. Used to attach accessories. This hole is used only for the purpose of attaching accessories.
    - Mounting hole size
      - 1/4-20 UNC (screw length 13 mm or shorter)
15. Lock release button
16. Used to release the lock of the V-groove.
17. V-groove
18. Used to attach the rear viewfinder.

Top of the page