- Top
- Maintenance
- Warning displays
- Other warning displays

Other warning displays

[FAN OFF] | Fan has stopped.
[UPDATE ERROR!] [ERRCODE:01] | The version update file is invalid. Store the correct version update file in the SD memory card, and the execute the update again.
[UPDATE ERROR!] [ERRCODE:02] | The version update file does not exist. Store the correct version update file in the SD memory card, and the execute the update again.
[UPDATE ERROR!] [ERRCODE:03] | Mounting error of the SD memory card. The SD memory card may not be inserted, or the SD memory card may be damaged.
[UPDATE ERROR!] [ERRCODE:04] | File load error. The SD memory card may be ejected during the version update, or the version update file in the SD memory card may be corrupted.
[UPDATE ERROR!] [ERRCODE:05] | An error has occurred during the ROM erase for overwriting the version update file. Consult the dealer.
[UPDATE ERROR!] [ERRCODE:06] | An error has occurred during the ROM write for overwriting the version update file. Consult the dealer.
[UPDATE ERROR!] [ERRCODE:07] | The version update file is invalid. Store the correct version update file in the SD memory card, and the execute the update again.
[UPDATE ERROR!] [ERRCODE:08] | Other system error. (Communication error, etc.) Consult the dealer.
[TEMP OVER!] [FORCE POWER OFF!!] | The internal temperature is high. The power is turned off forcefully. Operate the fan when set to [MAIN MENU] → [MAINTENANCE] → [FAN SETTING] → [FAN] → [FAN MODE] → [OFF].

Top of the page