- Top
- Description of Parts
- Right side

Right side

1. <OPT FIBER> terminal
2. Used to connect with the CCU using the optical fiber multi cable. When the terminal is not in use, attach the dust cap.
3. <LAN> terminal
4. Used to connect the LAN cable (100BASE-TX/1000BASE-T).

   NOTE The cable connected to the <LAN> terminal should be a category 5e or better STP (Shielded Twisted Pair) cable.

5. Shoulder pad
6. Reduces the burden on the shoulder when the camera is carried on your shoulder.
7. Slide lock release lever
8. Releases this lever when changing the shoulder pad position.
9. Shoulder strap fittings
10. Used to attach the shoulder strap.
11. <VF> terminal
12. Used to connect the plug of the viewfinder.
13. Camera number sheet holder
14. Attach the supplied camera number sheet.
15. <USER 3> button
16. A user-selected function can be assigned to this button. Pressing the button performs the assigned function.
17. <LENS> terminal
18. Used to connect the lens cable.

Top of the page